{"text_format":"2","workbook":"xls","n_sheets":32,"sheets":["Mobile_LCD","Renesas_ICs","HWK","Nokia","Orders","Arima","Wintek","Wistron","Shenzhen ","MJC","GEI","Adelco","EDT","DLC","KET","Repro","Mairong","CSTN","TFT","Monochrome","STE_ICs","Leadis_ICs","IST_ICs","Samsung_ICs","Driver_IC","Sources","LCD_Types","List2","Sharp","TD025THEA7","FORMATS","List1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":259,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Mobile_LCD","index":0,"n_rows":275,"n_cols":11,"rows_kept":275,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Make, model","Price, UAH","Size in inches","Resolution (X, Y) in pixels","Display marking and label on the cable","Controller and analogs","Type (bw / colour)","Interface (parallel / serial)","Num Pins","Flex cable or connector","Voltage (V)"]
["Alcatel 300 (with board and joystick) (BE4)",14,{"$nulls":6},23,"?"]
["Alcatel 301 (with board and joystick) (BE4)",14,{"$nulls":6},23,"?"]
["Alcatel OT301/OT302 (BE4)","3-","?","96x49","Similar to Samsung","KS0723 / S6B1713 ( equ SED1565 )","b/w","serial",26,"шлейф"]
["Alcatel 311 (BF3)",4,null,"96x65","7636A01EIP212016","SED15B1","b/w",null,18,"плата","2.8V"]
["Alcatel OT320 (XG1) aka LG B1200/B1300",4,"?",null,null,null,"b/w",null,28,"шлейф","?"]
["Alcatel OT331 (BG3)",4,null,"96x65","BG3-VLC B3 / SYE3922G2599","S1D15G14","color","serial SPI",18,"плата","2.8V"]
["Alcatel OT332 (BG3)",14,null,"112x64",null,null,"color","?",18,"плата","?"]
["Alcatel OT 500 / 700 (on board with joystick) (BE5)",14,null,"96x64",null,null,"b/w","?","?","?","?"]
["Alcatel OT501 (on board with joystick) (BE5)",14,null,"96x64",null,null,"b/w","?","?","?","?"]
["Alcatel OT511 (BF4)",4,null,"96x65","6657A02S1P10906B","S1D15B1","b/w","serial SPI",18,"плата","2.8V"]
["Alcatel OT525 (BG3)",14,null,"96x65",null,"SED15B1","b/w","serial SPI",18,"плата","2.8V"]
["Alcatel OT526 (BG3)",4,null,"96x65",null,null,"b/w","?","?",null,"?"]
["Alcatel OT556/557 (TH3)",14,null,"128x160","10070A01SNFS0613G","HD66766","CSTN 65k","parallel 16bit",32,"conn","2.8V"]
["Alcatel OT715 (BF5)",14,null,"100x150 (4GS)",null,null,"b/w","?",18,"плата","?"]
["Alcatel 835 (OH5) (2 display)",14,"1.8\" 1.2\"","128x160 + 128x160","TD018DREA1 / C143U182",null,"LTPS TFT","parallel ?",30,"conn","?"]
["Ericsson R600",4,null,"101x68",null,"SSD1850","b/w","parallel",30,"шлейф","?"]
["Ericsson T10 / T18",4]
["Ericsson T20 / T28 / T29","?"]
["LG B1200/B1300/ Alcatel 320",4,null,"112x64",null,null,"b/w","parallel",28,"шлейф","?"]
["LG C1100 / C1150 / C3100 / G1600 / G1610 ","?","?","128x128","LJ41-02032A UG12D205A/MAIN REV3.3(2)","S6B33B2","color CSTN 65k","parallel 16bit",34,"шлейф"]
["Mitsubishi Trium Mars (Neptun)",4,"1.33\"","96x65","HLM7601-100100","PCF8812","b/w","serial SPI",8,"шлейф","2.8V"]
["Mitsubishi MT-660 m21i","?","?","128x162","Sharp M129CP","HM17CM4096-03M","4096 colors","parallel","12+12","ribbon cable","2.8V"]
["Motorola 330 (glass)",12,null,"?",null,null,"b/w","?","?","?","?"]
["Motorola C113/C115/C116/C118/C123",16,null,"96x64","sch","ST7558","b/w FSTN","serial i2c",8,"шлейф","2.8V"]
["Motorola C139",40,"?","?",null,null,"color","serial",10,"шлейф"]
["Motorola C155/C156/C157/V171",44,null,"98x67","WD-X0906VF-6CLWe WM-X0906V4-6CLWa","UC1682","color STN","serial",10,"шлейф"]
["Motorola C210",14,null,"?",null,null,"b/w","?",18,"шлейф","?"]
["Motorola C257/C261/C271 (V177)",16,"1.8\"","160x128","WD-X1216WT-6CLW WD-X1216WF-6CLW TD018THEE3","sch ???","color TFT 65/262k","parallel",22,"conn","V_IO=2.8V"]
["Motorola С236/C250/C350/C450/C550 (with keyboard)",25,null,"96x65","LPH8592-1","SSD1770","color CSTN","serial","5+5","?","2.7V"]
["Motorola C168/C380/C385  /C390/C650/V180/V220 (interior)",22,null,"128x128","WD-X1313W","sch","color","?",20,"conn","2.7V"]
["Motorola K1/V3/V3i/W5/W510 (external)",14,null,"96x80","sch",null,"color","serial",9,"шлейф","?"]
["Motorola L2/L6",22,"1.8\"","160x128","QQVGA sch","?","color TFT","?",22,"conn","?"]
["Motorola L9/L72",null,null,"176x220",null,null,"color"]
["Motorola P7689/ Timeport250",2.42,null,"96x64","LCD with icon bar at the top","?","b/w","?","?","?","?"]
["Motorola T205",4,null,"96x65",null,"?","b/w","parallel",27,"шлейф","?"]
["Motorola T2288 Talkabout","?","?","?","?","?","b/w","?",16,"шлейф","?"]
["Motorola V180 complete assembly",38,"?","? + 32x96",null,"b/w ST7533","color + b/w"]
["Motorola V220 complete assembly",48,"?","? + 32x96",null,"b/w ST7533","color + b/w"]
["Motorola V235 (external)",14,null,"96x32","WD-G0903VF-6WNN",null,"b/w","?","?","шлейф","?"]
["Motorola V300/V400/V500/V525/V535 /V547/V600/V620 int.",31,null,"176x220",null,"?","color","?","?","?","?"]
["Motorola V360 (external)",14,null,"96x80 (4 gradations)","WD-G0908V","sch","b/w","serial",13,"шлейф","?"]
["Motorola V3688 (analogue V51)","4-",{"$nulls":6},20,"шлейф"]
["Motorola V50/V3690",8,null,"96x64","????","sch","b/w","parallel",18,"шлейф","?"]
["Motorola V51 (wide train)",22,null,"96x64",null,null,"b/w","?",20,"шлейф","?"]
["Motorola V60 (complete assembly on board)",14,null,"96x64",null,null,"b/w","?","?","conn","?"]
["Motorola V66",4,null,"96x64","sch",null,"b/w","?",25,"?","?"]
["Motorola V70",31,null,"96x64",null,null,"color",null,16,"conn"]
["Motorola W175 / W180 / W181",22,null,"128x128","WD-Y1212VP-6CLW1",null,"color","serial",12,"шлейф","?"]
["Motorola W220 (with dynamics)",22,null,"128x128","WD-X1313VB-6CLWc",null,"color","?",15,"conn","?"]
["Motorola W230",23,null,"128x128","WD-Y1212UC-60LWS",null,"color","?",22,"conn","?"]
["Motorola W370 / W375",61,"1.8\"","128x160","TD018THEJ8","???","color LTPS TFT","serial MicroWire",14,"шлейф","2.8V"]
["Nokia 1100 / 1101 / 2300 (glass)",20,null,"96x65","sch","PCF8814","b/w","serial SPI",9,"шлейф","?"]
["Nokia 1110i / 1112",16,"1.36\"","96x68","WD-G0906WY (1112) / WD-G0906YH (1110i) sch","STE9668D","b/w","serial",10,"conn","2.8V"]
["Nokia 1110 (glass)",17,null,"96x68","WD-G0906XH sch",null,"b/w","serial",10,"conn","2.8V"]
["Nokia 1116 / 1200 (similar to 1110 glass)",17,null,"96x68","sch",null,"b/w","serial",10,"conn","2.8V"]
["Nokia 1600 / 1208 / 1209 / 2310 / 2126 CDMA / (6125small / 6136 / N71small) external",28,"1.8\"","96x68","4850080 018LUE002 MP1.0 / 4850859 UG09B123AA","ST7628 LDS184","color CSTN 65k","serial",12,"conn"]
["Nokia 1616 / 1661 / 1662 / 1800 / 5030c / 1650",28,"1.8\"","128x160","WD-F1216XZ-6FLWd 4850266","S6B33D1 HX5081 NT39121","color TFT 65k","serial i2c",12,"шлейф"]
["Nokia 1680 Classic / 2600 Classic / 2630 / 2660 / 2760 / 3555 (copy)",32,null,"128x160","sch","SPFD54124","color TFT","serial i2c",24,"conn","?"]
["Nokia 1202/1203/1280",17,null,"96x68","no sch","STE2007 NT7542","b/w","serial",12,"шлейф","?"]
["Nokia 2100 (with keyboard)",42,{"$nulls":4},"b/w","serial",8,"шлейф"]
["Nokia 2220s / 2320 / 2323 / 2330 / 2680s / 2690 / 2720 / 3109c / 3110c / 3500 / 7070 (copy)",41,null,"128x160",null,"PCF8833? S1D15G00?","color"]
["Nokia 2270 (looks like 5110)","?",null,null,null,"OM6211","b/w"]
["Nokia 2760/6085/6086 (external)",22,null,"96x68","UG09B123AA  /  4850955  WD-G0906YJ-6NLBc 4850955","sch","color","serial",10,"conn","?"]
["Nokia 3100 / 3120 / 5100 / 6100 / 6600 / 6610 / 7200 / 7210 / 7250",32,null,"128x128","Epson","PCF8833 S1D15G10","color","serial SPI",10,"conn","2.8V & 1.8V"]
["Nokia 3109 / 3110 / 3500 Classic",41,"1.8\"","128x160","4850080 018LUE003 MP1.0 990000101","SPFD54124","TFT 262k","parallel",24,"conn","?"]
["Nokia 3155i / 6155 / 6155i",null,null,null,"Part No: 4850859"]
["Nokia 3210 / 3310 (glass) analogue 5110",16,null,"84x48","LPH7677 (3210)","PCD8544 / OM6206","b/w","serial",8,"glass"]
["Nokia 3410 / 3310 / 3210 / 5160 / 3350 / 3315",16,null,"84x48","LPH7779","OM6206 / PCF8812 / PCD8544","b/w","serial SPI",8,"glass","2.7V - 3.3V"]
["Nokia 3220 / 6020 / 6021 / 6235 / 7260 / 9300external / 9500 external / N90 external (copy)",48,null,"128x128",null,null,"color TFT",null,null,"conn"]
["Nokia 3230 / 6260 / 6630 / 6670 / 7610 (copy)",61,null,"176x208",null,"L2F50200 Epson","color","?","?","conn"]
["Nokia 3300 / 6800 / 6810",25,null,"128x128",null,"S1D15G10","color","?",10,"на плате","?"]
["Nokia 3360 / 3361 / 3320     / 1260 / 1261","?",null,null,"LPH7815-1","OM6217","b/w"]
["Nokia 3510 (with keyboard) (6510 / 8310)",17,null,"98x67",null,"OM6211 PCF8814","b/w","serial",8,"штырьки","2.7V & 1.8V"]
["Nokia 3510i / 3520 / 3530 / 3560 / 3595 (with keyboard)",17,null,"98x67","sch","S1D15G14 / PCF8835","color CSTN","serial",8,"на плате","?"]
["Nokia 3518","?",null,"?","?","?","b/w","?",14,"шлейф","?"]
["Nokia 5110 / 5130 / 6110 / 6150 / 8810 (with metal frame)",8,null,"84x48","LPH7366","PCD8544","FSTN b/w","serial SPI",9,"glass","2.7V - 3.3V"]
["Nokia 5210 (glass) /6210",17,null,"96x65","sch",null,"b/w","serial",8,"шлейф","?"]
["Nokia 5800w / 5800XM / 5802XM / 5228 / 5230 / 5233 / 5235 / N97 Mini / C6 / X6M",243,"3.2\"","360 x 640","LMS316CC01 4850096","HX8376-A  ILI9640  S6D05B0","LTPS TFT","serial",null,"шлейф"]
["Nokia 6030 / 2255 / 2610 / 2626 / 5140i",33,{"$nulls":4},"color","serial",10,"conn","?"]
["Nokia 6310 / 6310i",32,null,"96x64",null,"PCF8511","b/w","?","?","?"]
["Nokia 6101 / 6103 / 6170 / 7270 / 8910i (external)",20,null,"98x67","LPH9121T001","LDS184 / SPFD54124B?","color","serial","?","conn","?"]
["Nokia 6170 / 7270 interior",36,{"$nulls":4},"color","?","?","шлейф"]
["Nokia 6100 (written in box 3100)",40,null,"128x128","Also Leadis LDS176","S1D15G00 PCF8833","color","serial SPI",10,"conn","3.3V"]
["Nokia 6165 / 6165i","?","1.4\"","98x70","UG09B123AA / 4850859 MP1.0",null,"CSTN 65k","serial",10,"conn"]
["Nokia 6210",24,null,"96x60","LPH7690","PCD8544","b/w","serial SPI","?","?"]
["Nokia 6230",76,"1.5\"","128x128","LS015B8UA01C","Two chips","color","parallel",24,"conn","2.8V & 1.8V"]
["Nokia 6300 / 5320 / 6120C / 6350 / 6555 / 7500 / 8600",72,null,"240x320","sch",null,"color TFT","parallel",24,"conn","2.8V & 1.8V"]
["Nokia 6510 (glass) (pinout as 8310)",4,null,"84x48","sch","OM6211","b/w","serial",8,"шлейф","2.8V"]
["Nokia 7110","?",null,"96x65",null,"SED1565","b/w","serial",14,"conn на плате","3V"]
["Nokia 7390 (two displays)",90,"2.2\"",null,"4850985 MP1.02 / LS022Q3UT01M",null,"color",null,24,"conn"]
["Nokia 7650",68,null,"176x208","Epson L2F50006 (L2F50113T) series","MD 0046","color","parallel",30,"?","2.8V & 1.8V"]
["Nokia 8310 (pinout as 6510)",39,null,"84x48","?","OM6211","b/w","serial",8,"шлейф","2.8V"]
["Nokia 8850 / 8890",20,"?",null,"GPM291A1      NP4237-03",null,"color",null,26,"шлейф"]
["Nokia 8910 (very similar to 1110i)",4,null,"96x65(4GS)","01150P00204DP sch","?","b/w","serial",10,"conn"]
["Nokia 8910i / 7270 small / 6170 external / 6101 small /6103",20,"?","92x65","?","?","color 4096","serial",10,"conn"]
["Panasonic GD35",4,null,"84x48",null,null,"b/w","?","?","glass","?"]
["Philips 630 (2 displays)",22,null,"128x128 + 80x48",null,null,"color + b/w","?","?","?","?"]
["Sagem 3020",4,null,"96x64",null,null,"b/w","?","?","?","?"]
["Sagem MYX-1",16,"?","?",null,null,"b/w","parallel",21,"шлейф"]
["Sagem MYX-2",31]
["Sagem MYX-5M",31,"?","?","3L039973Q",null,"color","serial",10,"штырьки на плате"]
["Sagem MYX-6 / MYX-7",39,{"$nulls":4},"color",null,null,"шлейф"]
["Samsung 2400",16,null,"?","VG-T110651",null,"b/w","parallel",32,"шлейф","?"]
["Samsung A100",11,null,"?","VG-G120658",null,"b/w","parallel",33,"шлейф","?"]
["Samsung A100 (complete assembly)",16,null,"?",null,null,"b/w","parallel","?","шлейф","?"]
["Samsung A200 CDMA",11,null,"?",null,null,"b/w","parallel",31,"шлейф","?"]
["Samsung A200 CDMA (complete assembly two displays)",16,null,"?",null,null,"b/w","parallel","?","conn","?"]
["Samsung A300 (complete assembly with speaker and vibro)",16,null,"?",null,null,"b/w","?","?","conn","?"]
["Samsung A300 (interior)",11,null,"?",null,null,"b/w","parallel","~32","шлейф","?"]
["Samsung A460 CDMA interior","?","?","128x128 (4gs)","COF Display",null,"b/w","parallel",34,"шлейф"]
["Samsung A460 CDMA external","?","?","64x64","COF Display(TAB)",null,"b/w","parallel",32,"шлейф"]
["Samsung C130",null,null,"128x128","wd-x1212xl","S1D15G27"]
["Samsung C260/C160/C168/C450/C158 /B100/B200","?",null,"128x128","WD-Y1212VE",null,"color CSTN 65k",null,32,"шлейф"]
["Samsung C300B/X160B/X510","?",null,null,"UG12R225A  LJ41-04456A",null,"color"]
["Samsung D500E","?","1.9\"","176x220","LTS190QC-E02",null,"color TFT 262k","parallel 16bit",29,"шлейф"]
["Samsung D880 DUOS",null,null,"240x320","UG080729T21",null,"color","parallel",null,"плата+ conn"]
["Samsung N100",4,null,"?",null,null,"b/w","parallel","~32","шлейф","?"]
["Samsung N500",4,null,"?",null,null,"b/w","parallel","~32","шлейф","?"]
["Samsung R200/R210/R220",4,null,"132x65","R220","S6B0723","b/w","parallel",36,"шлейф","?"]
["Samsung GT-S5230","?","3.0\"","240x400","GT-S5230_REV0.2","S6D04D1","TFT 262k","parallel",31,"шлейф","2.9V"]
["Samsung X160/X200/X210","?","1.8\"","128x160","X210KAA6A2R007 UG12R215A",null,"color 65k",null,30,"conn","2.9V"]
["Samsung X600",null,null,null,"PFM7874","?","color","parallel",32,"шлейф"]
["Siemens A31/AX75/AX76/C72/C76/AX72",39,null,"128x128","LPH9135-3","LDS183","color","serial",10,"плата"]
["Siemens A35",4,"?","?","COF Display","?","b/w","?",30,"шлейф","?"]
["Siemens A50/C45/M50","24-","?","?","HP10514A","SSD1818A?","b/w","parallel","~20","шлейф","?"]
["Siemens A52/A55/A56/A57/C55","24-",null,"102x65","there is a description and source in C","PCF8812","b/w","serial SPI",8,"плата","2.8V"]
["Siemens A57","24-",null,"?",null,null,"b/w","?","?","?","?"]
["Siemens A60","57-",null,null,null,"S1D15G14","color"]
["Siemens A70/A71",52,null,"101x64","HP10534R","PCF8812/13","b/w","serial SPI",10,"плата"]
["Siemens A75",64,null,"?",null,null,"color","serial",10,"плата"]
["Siemens C35/M35",4,"?","?","?","SSD1818A?","b/w","serial",26,"шлейф"]
["Siemens C55 with keyboard",31,null,"101x64",null,null,"color"]
["Siemens C62 / SonyEricsson J300i",31,null,"128x128",null,null,"color",null,32,"шлейф"]
["Siemens C65",92,null,"130x130",null,"S6B33B2","color CSTN","?","?","?"]
["Siemens C75/ME75",76,null,"132x176","LPH9157-2",null,"color TFT",null,10]
["Siemens M75/CX75/M81/C81",56,null,"132x176",null,null,"color TFT",null,20,"плата"]
["Siemens S35","4-","?","?","?","?","b/w","?",26,"шлейф"]
["Siemens S40","4-","?","?","Looks like Samsung","COF","b/w","?",40,"шлейф"]
["Siemens S55/          M55/A60/A65/C60/MC60",56,null,"101x80","LPH8731-3C / LM15SGFNZ04 / LM15SGFNZ07","S1D15G14 LH15AB HM17CM4096","color CSTN",null,10,"плата"]
["Siemens S65/M65/CX65/SK65/CX70",105,null,"176x132","LPH8836-2 / LS020","L2F50126 / S1D13732??","color","serial SPI",10,"плата"]
["Siemens S75/SX75",80,null,"132x176",null,"PCF8882","color","parallel",20,"плата"]
["BenQ Siemens EL71/E71",80,null,"240x320",null,"JBT6K71","color TFT"]
["Sony Ericsson C510",88,"2.2\"","240x320",null,null,"TFT 262k",null,26,"conn"]
["Sony Ericsson T100","дог.","1.3\"","101x67 (4GS)","MM13G05A Arima","ST7568","b/w","parallel",30,"шлейф"]
["Sony Ericsson T105","?","1.3\"","101x67 (4GS)","MM13G05A Arima","ST7568","b/w","parallel",30,"шлейф"]
["Sony Ericsson T230/T290",22,null,"101x80","RNH 942213","UC1682s","color","serial i2c",8,"шлейф","2.85V"]
["Sony Ericsson T250/T280/K330",30,null,"160x128","RB377-10A R1A",null,"color",null,"16+17","шлейф"]
["Sony Ericsson T300/T310",31,null,"101x80","RNH94258/2 R1A","HD66760 / UC1682","color","serial i2c",8,"плата","2.8V"]
["Sony Ericsson T303",61]
["Sony Ericsson T68/T68i (very similar to T300 / T310)",31,null,"101x80","RNH94254/2 R2A A / RNH94254/2 R5A / MC16F01A Arima","HD66760 / UC1682","color CSTN","serial i2c",8,"плата","2.8V"]
["Sony Ericsson T610",46,"1.9\"","128x160","sch","HD66766","color 65k",null,23,"шлейф"]
["Sony Ericsson T630/T637",52,null,"128x160","RNH94264/2 / SXK1095990   /  G430B R1E   / G521E R1E","HD66773","color TFT",null,23,"шлейф"]
["Sony Ericsson T650i / K770",69,null,"240x320",null,"R61505U","color"]
["Sony Ericsson J100i",16,null,"96x64","LPH9349-1   / K0064H-FL sch","LDS184 ST7628","color CSTN","serial",10,"шлейф"]
["Sony Ericsson J105",60]
["Sony Ericsson J110i/J120i",18,null,"96x64","WD-X0906XQ / RNH1200 2104","PCF8833? / LDS184","color CSTN","serial",12,"шлейф"]
["Sony Ericsson J132",null,null,null,"UG12D247A CS1"]
["Sony Ericsson J200",38,null,"128x128","WD-X1212VV-7CLW9",null,"color",null,20,"conn"]
["Sony Ericsson J210i/J200/J210",39,"1.6\"","128x128","MC16G12B Arima","NT7525(71)","color CSTN","parallel",20,"conn","3V"]
["Sony Ericsson J220i/J230i",32,{"$nulls":4},"color"]
["Sony Ericsson J300i/ Siemens C62",20,null,"128x128","ODM37-80401A","?","color","parallel",32,"шлейф"]
["Sony Ericsson K200/K220",24,"1.6\"","128x128","RB370-10A R1A / MC16G23B Arima","S6B33BG","color CSTN","parallel",20,"шлейф","?"]
["Sony Ericsson K205/J132",31,null,null,"UG12D247A CS1",null,"color",null,14,"шлейф"]
["Sony Ericsson K300i",54,{"$nulls":4},"color",null,"?","шлейф"]
["Sony Ericsson K310i/K320i/W200",54,"2.0\"","128x160","ODM37-80405 / RB342-AG","R64500","color TFT","parallel 8 bit",24,"шлейф"]
["Sony Ericsson K500i",162,null,null,"RNH94263/7 Z",null,"color"]
["Sony Ericsson K510i",60,"2.0\"","128x160","RB342-AG","R65002","color","parallel 8 bit",24,"шлейф"]
["Sony Ericsson K530i","?",null,"176x220",null,"R61503","color"]
["Sony Ericsson K550i/K550im/W610i",52,null,"176x220","RNH80111 R2B","L2F50313T01","color"]
["Sony Ericsson K600i/K600i/K608i",70,null,"176x220",null,"EPSON L2F50313T01","color"]
["Sony Ericsson K610i/K610im / V630",113,null,"176x220",null,"R61503_T2J","color"]
["Sony Ericsson K630i",113,null,"176x220",null,"R61503","color"]
["Sony Ericsson K660i","113-",null,"240x320",null,"R61505U","color"]
["Sony Ericsson K700i",96,null,"176x240","RNH94227","HD66789R","color TFT","parallel",23,"шлейф"]
["Sony Ericsson K750/D750/W700/W800 with a green train",68,null,"176x220","RNH94229 R2C / RNH94229 R4A","HD66789R R61503_B1","color TFT","parallel",20,"шлейф"]
["Sony Ericsson K750i/D750/W700/W800 with a yellow train",72,null,"176x220","RNH94229 R2C / RNH94229 R4A","HD66789R R61503_B1","color TFT","parallel",20,"шлейф"]
["Sony Ericsson K770i / T650",69,null,"240x320",null,"R61505U","color",null,26]
["Sony Ericsson K790i/K800i/K810i/W830/ W850i",72,"2.0\"","240x320","RNH942268","R63400A1 JBT6K71","color",null,null,"шлейф"]
["Sony Ericsson K850i",69,null,"240x320",null,"R61505U","color"]
["Sony Ericsson M600 sensory","138-","2.6\"","240x320","sch",null,"262k"]
["Sony Ericsson P800 with touchscreen","267-",null,"208x320",null,null,"color 4k",null,"?"]
["Sony Ericsson P900 / P910 with touchscreen","227-",null,"208x320","sch",null,"TFT 262k"]
["Sony Ericsson P990i with touchscreen",63,null,"240x320","sch",null,"TFT 262k"]
["Sony Ericsson R300",42,"1.8\"","128x160","RB383-10 R1A",null,"TFT 65k",null,24,"conn"]
["Sony Ericsson S302 / W302",77,"2.0\"","176x220",null,null,"TFT 262k"]
["Sony Ericsson S312",80]
["Sony Ericsson S500i/W580 yellow train",54,null,"240x320",null,null,"color TFT 262k",null,24,"conn"]
["Sony Ericsson S500i/W580 with a green train",96,null,"240x320","sch",null,"color",null,24,"conn"]
["Sony Ericsson S700/S710",96,null,null,"sch",null,"color"]
["Sony Ericsson V600i","?",null,"176x220",null,"EPSON L2F50313T01","color"]
["Sony Ericsson V630i",113,null,"176x220",null,"R61503 T2J","color"]
["Sony Ericsson V640i","?",null,"176x220",null,"R61503","color"]
["Sony Ericsson W100 (Spiro)",61,"2.2\"","320x240",null,null,"TFT 262k"]
["Sony Ericsson W20 (Zylo)","130-"]
["Sony Ericsson W200i","?",null,"128x160",null,"R64500","color"]
["Sony Ericsson W205",54,"1.8\"","160x128","MP1217-2423 R1E",null,"TFT 65k",null,"~20","шлейф"]
["Sony Ericsson W300i (two LCD)",89,null,"128x160 101x108",null,"R61502 Second: R16500PA5","TFT262k + color"]
["Sony Ericsson W350",46,null,"176x220",null,null,"color 65k"]
["Sony Ericsson W380i/Z555 interior",46,null,"176x220",null,"S6D0164","color",null,null,"conn"]
["Sony Ericsson W380i external",54,null,null,null,"RIT","color"]
["Sony Ericsson W550i / W600",69,null,"176x220","sch","R61500 A","color"]
["Sony Ericsson W660i/K530/K630/K660/K830",60,null,"176x220",null,"R61503","color"]
["Sony Ericsson W700i","?",null,"176x220",null,"R61500 B","color"]
["Sony Ericsson W710i / Z710",218,null,"176x220",null,"S1D19111 Second: UC1617","color"]
["Sony Ericsson W760",44,"2.2\"","240x320","N8110007196",null,"color TFT 262k",null,24,"conn"]
["Sony Ericsson W810i",105,null,"176x220","sch","R61500 B S1D19111 D","color"]
["Sony Ericsson W850i","?",null,"240x320","sch","R63400A1 JBT6K71","color"]
["Sony Ericsson W880i",89,null,"240x320",null,"EPSON L5F30537 for FP23","color"]
["Sony Ericsson W890i / T700 / (K990)",47,null,"240x320",null,"EPSON L5F30728","color TFT 262k",null,26,"conn"]
["Sony Ericsson W900",null,null,"320x240",null,null,"TFT 262k"]
["Sony Ericsson Z200 external",20,"0.9\"","64x64","MM09G02A Arima / WD-G0606W","SSD0817","b/w","parallel",28,"шлейф"]
["Sony Ericsson Z200 interior",38,"1.6\"","128x128","MC16G03A Arima","SSD1781","color (CSTN)","parallel",null,"шлейф"]
["Sony Ericsson Z250i / Z320i",38,"1.8\"","128x160","LP-9399-G","S6B33BC","color TFT","parallel",23,"шлейф"]
["Sony Ericsson Z300 complete assembly (two displays color & b/w)",30,null,"128x128 64x64 b/w",null,null,"CSTN65k + b/w",null,null,"conn"]
["Sony Ericsson Z310i (module of two LCD)",38,null,"128x160 96x64 b/w",null,"STE2007 / S6B33BC","CSTN65k + b/w"]
["Sony Ericsson Z500 (Two LCDs)",47,null,"128x160 ???x???","WB-Z1216Y-6CLWI",null,"CSTN65k CSTN4k",null,24,"conn"]
["Sony Ericsson Z520i (Two LCDs)",54,null,"128x160 80x101","RNH94221 R1D","HD66773 Second: UC1682","CSTN65k CSTN4k",null,24,"conn"]
["Sony Ericsson Z525i (Two LCDs)",54,null,"128x160 80x101",null,"HD66773 Second: UC1682","CSTN65k CSTN4k"]
["Sony Ericsson Z530i (Two LCDs)",137,null,"128x160 101x80",null,"Second: R16500PA5","UBC65k",null,24,"conn"]
["Sony Ericsson Z550i","154-",null,"176x220",null,"R61503 Second: UC1617","color"]
["Sony Ericsson Z555i","?",null,"176x220",null,"S6D0164 Second: RIT","color"]
["Sony Ericsson Z558i",154,null,"176x220",null,"R61503 Second: UC1617","color"]
["Sony Ericsson Z610i (external)",22,null,"128x36","RNH94274 R2A",null,"OLED b/w",null,null,"шлейф"]
["Sony Ericsson Z610i (interior)",68,null,"176x220",null,null,"TFD 262k",null,null,"шлейф"]
["Sony Ericsson Z710i","?",null,"176x220",null,"S1D19111 Second: UC1617","color"]
["Sony Ericsson Z770i / Z780 (Two LCDs)",130,null,"240x320",null,"R61505U Second: BECKY_R61502"]
["Sony Ericsson Z800/V800 external",38,null,"101x80",null,null,"TFT 65k"]
["Sony Ericsson Z800/V800 interior",68,null,"176x220",null,null,"TFT 262k",null,null,"шлейф"]
[]
["NOKIA N95 copy 8K0023",89]
["TFT-8K0354-FPC-A1-E",89]
["TFT8K0486",null,"3.0\"",null,null,"SSD1289",null,null,37]
["TFT8K0561",null,"2.4\"",null,null,"R61501",null,null,37]
["NOKIA N95 copy 8K0561",89]
["NOKIA N95 copy 8K0594",89]
["NOKIA N95 copy 8K0669",153]
["TFT8K0762FPC-A1-E complete assembly",153]
["TFT8K0762FPC-A1-E glass",89]
["NOKIA N95 copy 8K1170",89]
["8K1201",89]
["TFT8K1201FPC-A1-E TRULY-C",89]
["TFT8K1358FPC-A1-E",null,"3.0\"",null,null,"R61505  ILI9325",null,null,37]
["TFT8K1465FPC-A1-E",89]
["NOKIA N95 copy 8K1486",89]
["NOKIA N95 copy TFT8K1596FPC-A1-E",89]
["TFT8K1658",null,"2.4\"",null,null,"ILI9320",null,null,37]
["TFT8K1670FPC-A1-E",89,"3.0\"",null,null,"R61505",null,null,37]
["TFT8K1749FPC-A1-E",89]
["TFT8K1937FPC-A1-E",89]
["TFT8K2108",113]
["TFT8K2188FPC-WQVGA-E1 with touchscreen",153]
["TFT8K2346FPC-A1-E",121]
["TFT8K2428FPC-A1-E(TRULY-C)",89]
["TFT8K2485FPC-A1-E",89]
["8K2825",97]
["8K2895",89]
["TFT8K3277FPC-A2-E",89]
["TFT8k3278FPC-A2-E",89]
["TFT8K3364FPC-A1-E",89]
[]
[]
[]
[]
[]
[{"$nulls":4},"LPH7319"]
[]
[]
["Promising models"]
["It makes sense to buy and use"]
["No point in messing around"]
["Available for experimentation"]
["Explore the data !!!"]
["Indicates color display (for convenience)"]
["sch - there is a scheme"]

{"sheet":"Renesas_ICs","index":1,"n_rows":58,"n_cols":6,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Renesas LCD Drivers",null,null,"Warning!"]
[]
[]
["Type","Resolution","Colors","Technology","Short Description","Format"]
["HD66740","112x80","b/w","STN"]
["HD66750S","128x128","b/w(4GS)","STN"]
["HD66753","132x168","b/w(4GS)","STN"]
["HD66760","104x80",256]
["HD66766","132x176","65k","Color STN",null,"QQVGA"]
["HD66766U","132x176","65k","Color STN",null,"QQVGA"]
["HD66767","132x132","4k","Color STN"]
["HD66768","104x84","4k","Color STN"]
["HD66773","132x176","65k","Amorphous TFT",null,"QQVGA"]
["HD66773R","132x176","65k","Amorphous TFT","Low Power","QQVGA"]
["HD66776+HD667P20","256x320"]
["HD66777","132x176 132x96 sub","262k","Amorphous TFT","Main & Subdisplay in one body"]
["HD66781S+HD66795","240x416",null,"Amorphous TFT","2-chip Set","WQVGA"]
["HD66782","132x132"]
["HD66784","176x200 96x96 sub",null,"Amorphous TFT","Main & Subdisplay in one body"]
["HD66784R","176x220 176x96 sub",null,"Amorphous TFT","Main & Subdisplay in one body"]
["HD66789R","176x240","262k",null,"Аналог R61500 по хар-кам","QCIF+"]
["HD66791","132x176","262k","Amorphous TFT",null,"QQVGA"]
["HD66795"]
[]
["R61201","176x240 (187x240)","262k","Amorphous TFT","For DSC (Digital Still Cameras)"]
[]
["R61402+HD66795","240x416","262k","Amorphous TFT","2-chip Set, MDDI Interface","WQVGA"]
["R61404+HD66795","240x416","262k","Amorphous TFT","2-chip Set, MDDI not supported","WQVGA"]
[]
["R61500","176x240",null,"Amorphous TFT",null,"QCIF+"]
["R61501","128x160","65k","Amorphous TFT"]
["R61502","128x160","262k","Amorphous TFT"]
["R61503","176x220","262k","Amorphous TFT"]
["R61503U","176x220","262k","Amorphous TFT"]
["R61504","240x320","16M","Amorphous TFT","MDDI Interface, 24 bit (Advanced R61505)","QVGA"]
["R61505","240x320","262k","Amorphous TFT",null,"QVGA"]
["R61505U","240x320","262k","Amorphous TFT",null,"QVGA"]
["R61506","176x132","262k(65k)","Amorphous TFT","Landscape Type","QQVGA"]
["R61507","128x128","65k"]
["R61508","128x160","262k","Amorphous TFT"]
["R61509","240x432"]
[]
[]
["R63400","240x360",null,"LTPS TFT",null,"QVGA"]
["R63401","320x240",null,"LTPS TFT","Landscape Type","QVGA"]
["R63402","320x240"]
[]
["R64500","132x176","65k","Color STN","Reduced chip size of HD66766U","QQVGA"]
[]
[]
[]
[]
[]
["LTPS - Low Temperature PolySilicon"]
["Amorphous TFT, reduced to 65k colors"]
["Color STN with 65k Colours"]
["Dual-chip versions"]
["Amorphous TFT with 262k Colours"]

{"sheet":"HWK","index":2,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["HWK Flasher"]
["Type",null,null,"Driver","Resolution","Cellphone models"]
["LCD Type:","PHI:","NAXvD6","LDS184","98(RGB)x70","Nokia 2310"]
[null,"PHI:","NAXv80","LDS184","98(RGB)x70","Nokia 1600"]
[null,"SDI:","NAXv86","LDS184","98(RGB)x70","Nokia 1208 1600"]
[null,"SDI:","NAXv87","LDS184","98(RGB)x70","Nokia 1200 1208 1600 2310"]
[null,"SDI:","NAXv88","LDS184","98(RGB)x70","Nokia 1208 1600 2310"]
[null,"SDI:","NAXv89","S6B33BD","98x70 RGB","Nokia 1208 1600"]
[null,"TPO:","NAXv80","LDS184","98(RGB)x70","Nokia 1200 1208 1209 1600 6120c"]
[null,"TPO:","NAXv8B","LDS184","98(RGB)x70","Nokia 1208 1600"]
[null,"SEID:","NAXvA2","S6B33BD","98x70 RGB"]
[]
[]
[null,"PHI:","LD184v8b"]
[]
[null,"SDI:","GUINv86","S6B33D1","128x160 RGB","Nokia 1616, 1650"]
[null,"WIN:","GUINvA0","STE2028","162x130 RGB","Nokia 1650"]
[]
[null,"SDI:","MYKSv00","STE9668D","96x68 Mono","Nokia 1110i 1202 1200"]
[null,"INLX:","MYKSv01","ST7506",null,"Nokia 1112"]
[null,"INLX:","MYKSv02","ST7506",null,"Nokia 1112i"]
[null,"INLX:","MYKSv03","ST7506",null,"Nokia 1200"]
[null,"INLX:","MYKSv08","ST7507",null,"Nokia 1200"]
[]
[]
[]
[null,"WIN:","MILSv00","ST7506",null,"Nokia 1110"]
[null,"SDI:","MILS00",null,null,"Nokia 1110"]
[]
[null,"WINTK:","SYRS01",null,null,"Nokia 1112"]
[]
[null,null,"SUEZ",null,null,"Nokia 6111",4850975]
[]
[null,"TPO:","BOHAIv80","HX5081",null,"Nokia 1616"]
["/SPFD54124","WIN:","BOHAIv91","NT39121",null,"Nokia 1661 1662"]
[null,"SDI:","BOHAIv92","NT39121",null,"Nokia 1661"]
[null,"INNO:","BOHAIv93","NT39121",null,"Nokia 1616 1800"]
[null,"WIN:","BOHAIv94","NT39121",null,"Nokia 1800"]
[]
["NT7542WH-DP1/3E","WIN:","SERI:8a","NT7542","96x68 Mono","Nokia 1202 1203"]
["NT75421H-D/3EF","WIN:","SERIv90","NT7542",null,"Nokia 1280"]
[null,"INLX:","SERIv91","NT7542",null,"Nokia 1202 1280"]
[]
[null,null,null,"SED15G10ITO",null,"Nokia 3100"]
[]
[null,"SEID:","S31va1"]
[]
[]
[null,null,"ST7506 ST7507 NT7542 NT39121 S6B33BD s6b33a0 STE2028 LDS184"]
["UC1698U"]

{"sheet":"Nokia","index":3,"n_rows":36,"n_cols":3,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
["Model","Description","Spare Part Number"]
[]
["Nokia 1110i/1112","LCD PM 96X68 COG BW Syros",4851020]
[null,"LCD PM FSTN 96X68 COG Mykonos",4850104]
[]
["Nokia 1110","LCD PM 96X68 FSTN BW MILOS",4850921]
[]
["Nokia 1200","LCD PM 96X68 COG BW Mykonos",4851030]
[null,"LCD PM 96x 68 COG Mykonos VE",4850106]
[null,"LCD PM FSTN 98X68 COG Mykonos",4850104]
[]
["Nokia 1208","LCD PM C-STN 98X70 COG NAXOS",4850110]
[null,"LCD PM 98x70 RGB CSTN COG Naxos VE",4851068]
[]
[]
["Nokia 1600","LCD PM 98x70 RGB CSTN COG Naxos VE",4851068]
[]
["Nokia 1650","LCD PM 128x160 COG 262k CSTN Guinea",4851042]
[null,"LCD PM 128x160 262k CSTN Guinea",4850190]
[]
["Nokia 2310","LCD PM 98x70 RGB CSTN COG Naxos VE",4851068]
[]
[]
["Nokia 6120c","LCD AM 240x320 16MCO Wulm",4850030]
[null,"LCD AM 240x320 16MCO Wulm",4851051]
[null,"LCD AM TFT LTPSi 240x320 16MCO Wulm",4851025]
[null,"LCD AM 240x320 16MCO WULM",4850124]
[null,"DISPLAY ASSY WULM",4850254]
[null,"LCD AM TFT LT P-Si 240x320 16MCO Wulm",4850224]
[]
["Nokia 6136","LCD MOD PM 98 x 70 RGB CSTN COG Naxos VE",4850009]
[null,"LCD  AM 128x160 262K CO Suez",4850863]
[]
["Nokia 6300","LCD AM TFT LTPSi 240x320 16MCO Wulm",4851025]
[null,"LCD AM TFT LT P-Si 240x320 16MCO Wulm",4850224]

{"sheet":"Orders","index":4,"n_rows":52,"n_cols":5,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"www.gsmserver.kharkov.ua (Kharkiv, st.Korolenko, 23)"]
[null,null,"Order №1"]
["№ п/п","Product code","Name","Price, UAH","delivery times (order on Wednesday)"]
[1,305,"Display for Alcatel 311",4.03,"on Friday (2 days)"]
[2,5131,"Display for Alcatel 331",4.03,"on monday (5 days)"]
[3,306,"Display for Alcatel 511",4.03,"now"]
[4,7837,"Display for Alcatel 556/557",14.5,"now"]
[5,325,"Mitsubishi Mars",4.03,"on Friday (2 days)"]
[6,353,"Display for Nokia 6510 стекло",4.03,"now"]
[7,363,"Display for Nokia 8910",4.03,"now"]
[8,811532,"Display for Sony Ericsson J110/J120",18.52]
[9,5139,"Display for Alcatel 835",14.5,"two displays"]
[10,7383,"Loop for Samsung X160/X210",19]
[]
[null,null,"Total:",90.7]
[]
[null,null,"Order №2"]
["№ п/п","Product code","Name","Price, UAH","delivery times (order on Wednesday)"]
[1,820425,"Loop for Samsung D880",46.98,"everything on Monday after 13-00"]
[2,7847,"Display for Motorola C261/C271/C257",16.2]
[3,3316,"Display for Alcatel 526",4.05]
[4,7838,"Display for Alcatel 715",14.58]
[5,9192,"Display for Sony Ericsson J100",16.11]
[]
[null,null,"Total:",97.91999999999999]
{"$rows_empty":10}
[null,null,"Not available"]
[null,326,"Display for Motorola P7689/Timeport250",2.42]
[null,343,"Display for Nokia 3510i/3530/3560/3520 с клавиатурой",17.72]
[null,6411,"Display for Nokia 5210 стекло",17.72]
[null,8384,"Motorola K1/V3/V3i/W5/W510 (внешний)",14.58]
[null,5660,"Display for Nokia 1600/1208/1209/2310/2126CDMA//(6125/6136/N71) внешний",28.35]
[]
[null,null,"На будущее"]
[null,919,"Display for Nokia 3300/6800/6810",25.77]
[null,3229,"Display for Sony Ericsson T230/T290",22.54]
[null,8617,"Motorola L2/L6",22.68]
[null,919,"Display for Nokia 3300/6800/6810",25.92]
[null,4163,"Display for Motorola C115/C116/C118/C123",16.2]
[null,5153,"Display for Philips 630",22.68,"Two displays"]
[null,365,"Display for Panasonic GD35",4.05,"Glass without leads"]
[null,813398,"Display for Sony Ericsson W760",44.55,"240x320"]
[null,813399,"Display for Sony Ericsson W890/T700",46.98,"240x320"]

{"sheet":"Arima","index":5,"n_rows":59,"n_cols":15,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,null,"Mobile applications"]
[null,null,"CSTN"]
["Size","Name","Resolution, pixels","Colour","Visible area, mm","Module size , mm","Pixel pitch, mm","Pixel size, mm","Brightness, cd / m 2","Display type","Interface","Controller","Supply voltage","Operating temperature range","Storage temperature"]
["1,0\"","MC10G03G","96RGB x 96","65K","20.92 x 20.8","27.0x45.6x2.75",null,null,190,"Tm",null,"ST7624-G","3,0V"]
["1.1\"","MC11G03B ","96(RGB)x96","65K","20.435x20.435","27.0x33.8x2.75","0.213x0.213","0.058x0.213",190,"CSTN","16 pins","ST7625","2.8V","-20°C~70°C","-30°C~80°C"]
["1,3\"","MC13G03B","128RGBx128","4K","30.0 x 22.00","37.0x50.0x5.5",null,null,90,"Tm","F.P.C 1.0mm_ Pitch 28 Pin","S6B33A2A02","3,0V"]
["1,3\"","MC13G08G","98RGBx67","4K","30.9 x 22.08","37.0x34.0x4.9",null,null,150,"Tm","F.P.C 0.8mm_ Pitch 24 Pin","UC1681","3,1V"]
["1.3\"","MC13G10B ","96(RGB)x64","65K","28.212x18.804","38.4x33.3x2.85","0.294x0.294","0.282x0.282",230,"CSTN","Serial Peripheral Interface","ST7628","1.8V;2.8V","-20°C~70°C","-30°C~80°C"]
["1.4\"","MC14G05A ","102x3(R.G.B)x80","65K","29.53x24.27","40.7x37.76x5.5","0.09x0.281","0.08x0.271",80,"CSTN","80 Series MPU 8-Bit Parallel","ST7625","2.6V-2.9V","-20°C~70°C","-30°C~80°C"]
["1,5\"","MC15G29B","128RGBx128","65K","28.52 x 30.1","38.4x42.9x3.8",null,null,80,"Tm","F.P.C 0.8mm_ Pitch 18 Pin","ST7636R-G"]
["1,5\"","MC15G31B","128RGBx128","65K","28.52 x 30.1","37.0x42.8x2.45",null,null,130,"Tm","8080 Series Parallel","UC1697","2,8V"]
["1,5\"","MC15G32G","128RGBx128","65K","28.3 x 30.17","33.35x41.64x3.0",null,null,160,"Tm","F.P.C 0.8mm_ Pitch 33 Pin","S6B33B6"]
["1.5\"","MC15G35B ","128RGBx128","65K","29.3x29.9","33.8x40.74x2.7","0.068x0.21","0.053x0.195",null,"CSTN","80/68 Series MPU 8/16-Bit Parallel","ST7637","2.8V","-20°C~70°C","-30°C~80°C"]
["1,6\"","MC16F01A",{"$nulls":7},"CSTN",null,"HD66760 / UC1682","2,8V"]
["1,6\"","MC16G12B","128RGBx128","65K","32.0 x 31.0","37.3x43.27x3.8","0.225x0.075","0.205x0.062",150,"Tm",null,"NT7525(71)","3,0V"]
["1,6\"","MC16G16H","128RGBx128","65K","32.0 x 31.0","38.0x43.16x3.55","0.225x0.075","0.205x0.062",-120,"Tm",null,"NT7571","3,0V"]
["1.6\"","MC16G23B","128RGBx128","65K","30.78x30.78","40x43.3x3","0.075x0.225","0.062x0.205",150,"CSTN","80 Series MPU 8-Bit Parallel","S6B33BG","1.8V;2.8V","-20°C~70°C","-30°C~80°C"]
["1,8\"","MC18G05G","128RGBx128","65K","30.54 x 36.04","38.40x47.1x3.9","0.073x0.219","0.061x0.207",-180,"Tm","8080 Series Parallel","S6B33B9","2,8V"]
["1.8\"","MC18G07G ","128RGBx160","65K","30.54x36.04","34.7x46.7x3.2","0.073x0.219","0.061x0.207",200,"CSTN","6800 Series Parallel/8 Bit","S6B33BC","2.9V","-20°C~70°C","-30°C~80°C"]
["1,9\"","MC19F01A","120RGBx160"]
["1,9\"","MC19G02B"]
["1.86\"","EDMMRG2KAS ","128RGBx160","65K","32.05x40.20","51.5x37.85x5.8","0.077x0.231","0.067x0.221",150,"CSTN","80CPU","NT7553","4.6V;7.0V","0°C~50°C","-30°C~60°C"]
["2.0\"","EDMMRG3KAS ","132 RGBx176","65K","29.685x39.585","58.3x40.2x7.9"," ",null,150,"CSTN",null,null,"4.6V","0°C~50°C","-30°C~60°C"]
["2.5\"","EDMMRF7KBS","132 RGBx176","65K","53.6x41.9","68.2x48.1x7.6"," ",null,150,"CSTN",null,null,"3.45V","0°C~50°C","-30°C~60°C"]
["2,8\"","MC28G01G"]
["2,8\"","MC28G02G"]
["2,8\"","MC28G03G","320RGBx240",{"$nulls":6},"CSTN","20 pin","?"]
["3,9\"","MC39G01B"]
["3,9\"","MC39T01B","320RGBx240","4096/65K","(82.8) x (62.8)","103.7x76.8x6.3",null,null,70,"Tm",null,"?","3,3V"]
["3,9\"","MC39T01H"]
["3,9\"","MC39T02H","320RGBx240","4096/65K","(82.8) x (62.8)",null,null,null,70,"Tm",null,"?","3,3V"]
[]
[]
[null,null,"Industrial applications"]
[null,null,"CSTN"]
[]
[null,null,"Mobile Application TFT"]
[null,null,"TFT"]
["Size","Name","Разрешение, точек","Цвет","Видимая область, мм","Размер модуля , мм","Шаг пикселей, мм","Размер пикселя, мм","Яркость , cd / m 2","Тип дисплея","Интерфейс","Контроллер","Напряжение питания","Диапазон рабочих температур","Температура хранения"]
["1.8\"","MT18G10G ","128(RGB)x160","262K","28.416x35.52","34.0 x47.0x2.3","0.074x0.0222"," ",220,"TFT","80 system CPU I/F 8 bits","HX-8310A","1.8 ~3.3 V","-20°C~60°C","-30°C~80°C"]
["1.8\"","MT18G13G ","176(RGB)x220","262K","28.512x35.64","34x47x2.5"," ","0.0162x 0.0162",200,"TFT","8/16-bit bus interface 80-system","ILI9221","2.4V ~ 3.3V","-20°C~70°C","-30°C~80°C"]
["2.0\"","MT20G07B ","176(RGB)x220","262K","31.68x39.6","38.18x53.32x2.65","0.06x0.018"," ",170,"TFT","80 system 8 bits","ILI9220","3.0V","-20°C~70°C","-30°C~80°C"]
["2.2\"","MT22G07B ","240(RGB)x320","65K","33.48x44.64","38.18x53.32x2.65","0.0155x0.1395",null,170,"TFT","80 system 8birs for 65K colors","HX8312A","3.0V","-20°C~70°C","-30°C~80°C"]
["2.4\"","MT24G01B","480x234","262K"," ",null,null,null,300,"TFT",null,null,null,"-20°C~70°C","-30°C~80°C"]
["2.4\"","MT24G03B ","240x320"," ","36.72x48.96","42.6x60.65x2.65"," ","0.153xRGBx0.153",250,"TFT","80-system 16 bit","ILI9320"," ","-20°C~70°C","-30°C~80°C"]
["2.8\"","MT28G01B ","240x320","262K","43.2x57.6","52.9x72.7x3.9","0.18x0.18"," ",200,"TFT","Parallel digital RGB","S6D0139","2.8V","-20°C~70°C","-30°C~80°C"]
["3.5\"","MT35G01B","320x240","FULL COLOR","70.08x52.56","76.9x63.9x4.5","0.073x0.219"," "," ","TFT","Digital RGB",null,"7.0V","-20°C~70°C","-30°C~80°C"]
["4.3\"","MT43G01B V5 (without t/p)","480x272","16M","95.04x53.856","105.5x67.2x2.9",null,"0.066x0.198",400,"TFT","R.G.B. Interface",null,"3.3V","-20°C~70°C","-30°C~80°C"]
["4.3\"","MT43G01G V1 (with t/p)","480x272","16M","95.04x53.856","105.5x67.2x2.9",null,"0.066x0.198",260,"TFT","R.G.B. Interface",null,"3.3V","-20°C~70°C","-30°C~80°C"]
[]
[]
[null,null,"ARIMA"]
[null,null,"MSTN"]
["Size","Name","Разрешение, точек","Цвет","Видимая область, мм","Размер модуля , мм","Шаг пикселей, мм","Размер пикселя, мм","Яркость , cd / m 2","Тип дисплея","Интерфейс","Контроллер","Напряжение питания","Диапазон рабочих температур","Температура хранения"]
["1.3\"","MM13G05H ","101RGBx67","Black/White","32.5 x 21.5","38.6x33.6x5.1","0.275 x 0.275","0.26 x 0.26",null,"MSTN","FPC /28 pins","ST 7568","3.0 V","-20°C ~70°C","-3 0°C~80°C"]
["1.4\"","MM14G05A ","96RGBx64","Normal White","32.77 x 24","40.7x52.8x5.5","0.315x0.315","0.3x0.3",null,"MSTN","80 Series MPU 8-Bit Parallel","SSD1829","2.8 V","-20°C ~70°C","-3 0°C~80°C"]
["1.7\"","MM17T01A ","128RGBx80","Black/White","38.5x24.78","44.5x66.9x 7.9","0.26x0.26","0.28x0.28",null,"MSTN","FPC / 18pins 0.5mmPitch","TL0350F3","7.0 V","-20°C ~70°C","-3 0°C~80°C"]
["5.7\"","EDMMUG1WAF ","320RGBx240",{"$nulls":6},"MSTN"]
["8.9\"","EDMGU95WFF","640RGBx240",{"$nulls":6},"MSTN"]

{"sheet":"Wintek","index":6,"n_rows":14,"n_cols":9,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Format","Model","Dimensions (WxH) mm","Visible area (WxH) mm","Pixel size (WxH) mm","Pixel pitch (WxH) mm","Backlight (LED)","Controller type","Colour"]
["128X128","WB-X1212V8-6CLWa","37x43.57x4.85","30.787x30.78","0.062x0.21","0.075x0.225","+","NT7525","65K"]
["128X128","WB-X1212V9-6CLWa","37x43.57x5","30.787x30.78","0.062x0.21","0.075x0.225","+","NT7525","65K"]
["128X160","WB-X1216V1-6CLWc","35.34x47.2x4.75","30.03x37.04","0.061x0.207","0.073x0.219","+","S6B33B2","65K"]
["128X160","WB-X1216V2-6CLWc","35.34x47.2x4.75","30.03x37.04","0.061x0.207","0.073x0.219","+","S6B33B2","65K"]
["96X64","WM-X0906V4-6CLWa","28x37.25x4.245","22.2x15.7","0.058x0.195","0.07x0.21","+","UC1682","4K"]
["128X128","WM-X1212VY-6CLWa","33.35x56.85x3.3","28.3x30.17","0.058x0.21","0.068x0.22","+","S1D15G27","65K"]
["128X160","WM-X1216V4-6CLWc","35.34x47.2x5","30.03x37.04","0.061x0.207","0.073x0.219","+","S6B33B2","65K"]
["128X160","WM-X1216V5-6CLWb","35.34x47.2x5","30.03x37.04","0.061x0.207","0.073x0.2319","+","S6B33B2","65K"]
["160X160","WM-X1616W-1CLWa","61.8x69.1x4.2","51.38x51.38","0.087x0.271","0.097x0.291","+","ST8016","By Controller"]
["128X96","WM-Y12091-6CLWe","38.8x53.8x7.1","32x26","0.213x0.2","0.225x0.225","+","HM17CM4096","4K"]
["128X128","WM-Y1212W-6CLWb","23.3x29.7x3.11","18.2x19.88","0.107x0.12","0.122x0.135","+","ST7528","4K"]
["128X128","WM-Z1212Y-6CLWa","37x58.07x3.28","30.787x30.78","0.062x0.205","0.075x0.225","+","NT7525","65K"]
["128X128","WM-Z1212Z-6CLWa","37x58.07x3.28","30.787x30.78","0.062x0.205","0.075x0.225","+","NT7525","65K"]

{"sheet":"Wistron","index":7,"n_rows":13,"n_cols":10,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Wistron Optics"]
[]
["Num","P/N","LCD Panel Part No","Size (inch)","Resolution","Type","Colors","Controller","N/Pins","Price $"]
[null,"143440-A 3.0"]
[1,"145710-A","T28QT7132",3.4,"240x320","TFT","16M",null,null,5]
[2,"145711-A",{"$nulls":5},"ILI9320"]
[3,"145712-A"]
[4,"145713-A","T28QT7132",3.4,"240x320","TFT","16M","ILI9325",null,5]
[5,"145714-A","T28QT7132",3.4,"240x320","TFT","16M","ILI9325",null,5]
[6,"145715-A",null,3.4,"240x320","TFT","16M",null,null,5]
[7,"145716-A",null,3.4,"240x320",null,null,"ILI9325",37]
[8,"145717-A",null,3.4,"240x320"]
[9,"146590-B","15564231E",2.8,"240x320","TFT","256k",null,null,15]

{"sheet":"Shenzhen ","index":8,"n_rows":4,"n_cols":7,"rows_kept":4,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["128x128","LCM","CSTN","RM4692/RM5095/RM5227","1,4\"","PCF8833/SSD1770Z/NT7571","4K/4K/65K"]
["98x67","LCM","CSTN","RM4983/RM5148/RM5254 /RM5337","1,33\"","SSD1770Z/EV65570/SSD1776 /ST7626","4K/65K/65K /65K"]
["96x64","LCD Module","CSTN","RM4830/RM5203/RM5425","1,1\"","SSD17882/PCF8835AU /UC1681S","65K/4K/4K"]
["128x160","LCD Module","CSTN",null,"1,8\""]

{"sheet":"MJC","index":9,"n_rows":82,"n_cols":9,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["CSTN"]
["Part NO. ","Size(Inch) ","Driver IC ","Color ","Active Area ","OutLine Dimension ","Resolution ","Backlight "]
["GWMC5494 ","1.77\" ","S6B33BC ","65K ","28.02*35.28 ","34.7*60.2*2.9 ","128*160 ","2-3Leds "]
["GWMC5411 ","1.51\" ","S6B33B6 ","65K ","26.1X28.14 ","33.3*41.6*2.9 ","128*128 ","3 Leds "]
["GWMC5513 ","1.51\" ","S6B33B6 ","65K ","26.1X28.14 ","33.3*41.6*2.9 ","128*128 ","1 Leds "]
["GWMC5002 ","1.51\" ","NT7525 ","65K ","26.1X28.14 ","33.3*41.6*2.9 ","128*128 ","3 Leds "]
["GWMC4824 ","1.51\" ","SSD1779 ","65K ","26.1X28.14 ","33.3*41.6*2.9 ","128*128 ","3 Leds "]
["GWMC5678 ","1.47\" ","S6B33BG ","65K ","26.1*26.867 ","33.35*41.6*2.25 ","128*128 ","2 Leds "]
["GWMC5689 ","1.47\" ","S6B33BG ","65K ","26.1*26.867 ","33.35*41.6*2.25 ","128*128 ","2 Leds "]
["GWMC5559 ","1.47\" ","UC1697 ","65K ","26.1*26.867 ","33.35*41.6*2.25 ","128*128 ","2 Leds "]
["GWMC5526 ","1.4\" ","NT7573 ","65K ","28.3*28.4 ","33.3*41.6*3.0 ","128*128 ","1 Leds "]
["GWMC5555 ","1.4\" ","S6B33BG ","65K ","28.3*28.4 ","33.3*41.6*3.0 ","128*128 ","1 Leds "]
["GWMC4983 ","1.33\" ","SSD1770Z ","65K ","27.92*19.082 ","37.0*34.0*3.0 ","98*67 ","1 Leds "]
["GWMC5337 ","1.33\" ","ST7626 ","65K ","27.92*19.082 ","37.0*34.0*3.0 ","98*67 ","1 Leds"]
[]
["Model NO. ","IC","Dimension","Dots","Color","PIN Description ","Interface"]
["CM5003","SSD1778 ","1.1\" ","96X64","65K","20PIN","6800/8080"]
["CM5004","LDS176A","1.5\" ","130X130","4K","10PIN","Series"]
["CM5005","UC1687 ","1.3\" ","128X96","65K","20PIN",8080]
["CM50006-01","UC1697 ","1.5\" ","128X128","65K","20PIN",8080]
["CM50006-03","UC1697 ","1.5\" ","128X128","65K","27PIN",8080]
["CM50008","S6B33B2 ","1.96\" ","128X160","65K","40PIN","6800/8080"]
["CM50010","NT7571-BDT","1.5\" ","128X128","65K","20PIN",8080]
["CM50011-01","NT7571-BDT","1.48\" ","128X128","65K","20PIN",8080]
["CM50011-03","NT7571-BDT","1.48\" ","128X128","65K","27PIN",8080]
["CM50012","HDC1600","1.8\" ","128X160","65K","20PIN",8080]
["CM50002-01","S6B33BC","1.8\" ","128X160","65K","20PIN",8080]
["CM50002-02","S6B33BC","1.8\" ","128X160","65K","28PIN",8080]
["CM50002-03","S6B33BC","1.8\" ","128X160","65K","30PIN","6800/8080"]
[]
["TFT"]
["Part NO. ","Size(Inch) ","Driver IC ","Color ","Active Area ","OutLine Dimension ","Resolution ","Backlight "]
["GWMF5549 ","3.5\" ","HX8218+HX8615 ","265K ","70.08*52.56 ","79.60*63.583*3.0 ","320*240 ","4 Leds "]
["GWMF5619 ","2.4\" ","HX8312 ","265K ","36.72*48.96 ","42.6*60.8*2.7 ","240*320 ","4 Leds "]
["GWMF5620 ","2.2\" ","HX8312 ","265K ","33.48*44.64 ","40.3*58.1*2.85 ","240*320 ","3 Leds "]
["GWMF5756 ","2.2\" ","HX8309 ","265K ","33.48*44.64 ","40.3*58.1*2.85 ","176*220 ","3 Leds "]
["GWMF5753 ","2.2\" ","R61503 ","265K ","33.48*44.64 ","40.3*58.1*2.85 ","176*220 ","3 Leds "]
["GWMF5629 ","2.0\" ","R61500 ","265K ","31.68*39.6 ","38.4*51.4*2.3 ","176*220 ","3 Leds "]
["GWMF5621 ","2.0\" ","HX8309 ","265K ","31.68*39.6 ","38.4*51.4*2.3 ","176*220 ","3 Leds "]
["GWMF5673 ","1.9\" ","HX8309 ","265K ","29.832*37.29 ","35.61*49.8*2.3 ","176*220 ","3 Leds "]
["GWMF5697 ","1.9\" ","ILI9220 ","265K ","29.832*37.29 ","35.61*49.8*2.3 ","176*220 ","3 Leds "]
["GWMF5563 ","1.8\" ","HX8310 ","265K ","28.416*35.52 ","33.9*46.65*2.9 ","128*160 ","3 Leds "]
["GWMF5733 ","1.8\" ","ILI9160 ","265K ","28.416*35.52 ","33.9*46.65*2.9 ","128*160 ","3 Leds "]
["GWMF5677 ","1.77\" ","S6D0144 ","265K ","28.032*35.04 ","34*44*2.75 ","128*160 ","2 Leds "]
["GWMF5747 ","1.5\" ","ILI9132 ","265K ","26.112*28.16 ","33.3*41.6*2.9 ","128*128 ","2 Leds "]
["GWMF5746 ","1.5\" ","ST7712 ","265K ","26.112*28.16 ","33.3*41.6*2.9 ","128*128 ","2 Leds"]
[]
[]
["Model No. ","Size ","Format ","Module Size ","Viewing Area ","DIGITAL /ANALOG "]
["SAT128128AD15","1.5\" ","128*128 ","31.7*52.7*3.6 ","26.112*28.16 "]
["SAT176220AA20","2.0\" ","176*220 ","38*64.1*3.0 ","33.68*41.4 "]
["SAT320240AC22 ","2.22\" ","320*234 ","40.70*57.70*2.7 ","34*46.14 ","DIGITAL "]
["SAT320234AB50","5.0\" ","320*234 ","119.3*91.4*7.5 ","102.72*74.53 ","ANALOG "]
["SAT320234AA56 ","5.6\" ","320*234 ","126.5*100.0*5.7 ","113.28*84.708 ","ANALOG "]
["SAT320240AB35 ","3.5\" ","320*240 ","76.9*63.9*4.4 ","70.08*52.56 "]
["SAT320240AG35 ","3.5\" ","320*240 ","76.9*63.9*3.4 ","70.08*52.56 ","DIGITAL "]
["SATTSR40825 ","3.5\" ","320*240 ","76.9*63.9*4.4 ","70.08*52.56 "]
["SAT320240AA57 ","5.7\" ","320*240 ","131*102.2*10.9 ","115.2*86.4 ","DIGITAL "]
["SAT400234AA65 ","6.5\" ","400*234 ","157.2*89.7*8.0 ","143.4*79.3 "]
["SAT480234AA25 ","2.5\" ","480*234 ","59.9*50.4*4.2 ","49.2*38.14 ","ANALOG "]
["SAT480234AC35 ","3.5\" ","480*234 ","83.0*60.5*3.3 ","72.0*50.544 ","ANALOG "]
["SAT480234AB35 ","3.5\" ","480*234 ","83.0*60.5*3.3 ","72.0*50.544 "]
["SAT480234AC70 ","7.0\" ","480*234 ","164.9*100*5.5 ","154.08*86.58 ","ANALOG "]
["SAT480272AA40 ","4.0\" ","480*272 ","98.3*62.6*5.4 ","87.84*49.776 "]
["SAT640480AA64 ","6.4\" ","640*480 ","145.5*111.5*6.0 ","130.56*97.92 "]
["SAT800480AA70 ","7.0\" ","800*480 ","165*104*5.5 ","152.4*91.44 ","DIGITAL "]
["SAT800480AA80 ","8.0\" ","800*480 ","192.8*116.9*6.4 ","176.64*99.36 ","DIGITAL "]
["SAT800600AA84 ","8.4\" ","800*600 ","203.0*142.5*7.5 ","170.4*127.8 "]
["SAT960240AA25 ","2.5\" ","960*240 ","60*52*3 ","50.88*38.16 ","DIGITAL "]
[]
[]
[]
[]
["COG"]
[]
["96*48 ","CBG964820J ","COG ","32.0*27.30","20.3*2.1 ","28.0*16.3 ","0.25*0.27 ","0.27*0.29 ","STE2002"]
["96*48 ","CBG964821J ","COG ","36.0*31.8","25.2*2.1 ","33.0*22.0 ","0.27*0.36 ","0.29*0.38 ","STE2002"]
["96*64 ","CBG966420K ","COG ","25.8*25.8","19.8","22.8*16.8 ","0.185*0.2 ","0.21*0.225 ","SSD1815BZ"]
["96*64 ","CBG966421A ","COG ","27.0*30.2","23.7*0.55 ","22.0*19.7 ","0.2*0.20 ","0.215*0.215 ","ST7565V-G"]
["96*64 ","CBG966422A ","COG ","34.2*29.0","22.5*0.7 ","30.5*20.5 ","0.261*0.261 ","0.281*0.281 ","ST7549"]
["96*64 ","CBG966423J ","COG ","36.0*31.8","25.2*2.1 ","33.0*22.22 ","0.265*0.265 ","0.285*0.285 ","S6B0721"]
["96*64 ","CBG966424J ","COG ","42.0*38.5","/46.0*2.1 ","39.0*35.5 ","0.32*0.43 ","0.37*0.48 ","S1D15605"]

{"sheet":"GEI","index":10,"n_rows":17,"n_cols":13,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["GEI LCD"]
["CSTN"]
["LCM NUMBER","SIZE inches","DOTS or PIXELS WxH","VIEWING AREA W x H in mm","LCM SIZE W x H x D in mm","DRIVER","-","COLOR","B/L","MAIN","DATA","PINS","VIEW Angle"]
["GTM9696AKHWG12-1","1.04\"","96 x 96","18.71 x 18.71","23.92 x 28.9 x 1.25","S6B33B5","MP","65K","without","CPU",8,39,"6:00"]
["GTM9664FKFWG-3","0.95\"","96 x 64","20.15 x 13.43","28.00 x 27.25 x 3.25","UC1681S","ES","65K","LED","CPU",8,24,"6:00"]
["GTM128160YKFWG","1.72\"","128 x 160","23.25 x 34.07","34.7 x 46.7 x 3.2","S6B33BC","MP","65K","P2LED","CPU",16,28,"6:00"]
["GTM128160YKFWG2","1.72\"","128 x 160","23.25 x 34.07","34.7 x 47.7 x 3.0","S6B33BC","MP","65K","S2LED","CPU",8,20,"6:00"]
["GTM128128B0KFWG","1.5\"","128 x 128","26.1 x 28.15","33.35 x 58.33","HDC1400 (SFD)","PP","65K","LED","CPU",null,null,"6:00"]
["GTMBP128128CKFWG39-9","1.5\"","128 x 128","26.1 x 28.15","34.8 x 41.5 x 1.8","S6B33B6","ES","65K","LED","CPU",null,null,"6:00"]
["GTM128128CKFWG32-9","1.5\"","128 x 128","26.1 x 28.15","33.4 x 41.6 x 3.0","S6B33B6","MP","65K","LED","CPU",16,32,"6:00"]
["GTM128128CKFWG40-10 ","1.5\"","128 x 128","26.1 x 28.15","33.4 x 41.6 x 3.0","S6B33BG","MP","65K","LED","CPU",16,32,"6:00"]
["GTM10280BKFWG2-1","1.4\"","102 x 80","27.53 x 22.47","36.5 x 35.6 x 3.3","UC1682S","MP","65K","LED","CPU",8,22,"6:00"]
["GTM9867AKFWG-1","1.33\"","98 x 67","27.92 x 19.08","36.2 x 33.3 x 3.4","UC1681S","PP","65K","LED","CPU",8,20,"6:00"]
["GTM128160LKFWG5-1","1.76\"","128 x 160","28.02 x 35.03","34.07 x 46.7 x 3.3","S6B33BC","MP","65K","LED","CPU",16,30,"6:00"]
["GTM128160VKFWG4","1.76\"","128 x 160","28.02 x 35.03","34.7 x 46.7 x 2.55","S6B33BC","MP","65K","P2LED","CPU",16,30,"6:00"]
["GTM128160WKFWG","1.76\"","128 x 160","28.02 x 35.03","34.00 x 46.6","HDC1600 (SFD)","PP","65K","LED","CPU",null,null,"6:00"]
["GTM176220IKFWG","1.89\"","176 x 220","28.50 x 35.63",null,"HDC1700 (SFD)","PP","262K","LED","CPU",null,null,"6:00"]

{"sheet":"Adelco","index":11,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["CSTN "]
["COLOUR ","MODULES"]
["Part Number","Size (inch)","Dot Format","Active Area (mm)","Outline Size (mm)","Driver","Color","Backlight","I/O","View Angle"]
[]
["MI9664HK","0.95","96x64","20.15x13.43","25.95x25.33","ST7628S","65K","LED","8 bit Parallel","6.00"]
["TM9664A2KFWG","0.95","96x64","13.43x20.12","27.72x28.0","ST7628","65K","LED","8 bit Parallel","6.00"]
["MI9664GK","1.00","96x64","20.15x13.43","24.60x25.50","ST7628-G","56K 260K","LED","8 bit Parallel","6.00"]
["MI9696FK","1.04","96x96","18.71x18.71","25.72x30.30","S6B33B5","65K","LED","Parallel","12.00"]
["MI13280AK","1.43","132x80","31.67x27.99","42.80x24.5","S6B33BG","65K","LED","CPU","6.00"]
["MI128128XK","1.44","128x128","25.49x26.49","32.36x53.3","ST7687S","65K","LED","CPU","6.00"]
["TM128128A4KFWG","1.44","128x128","25.5x26.5","33.35x41.64","ST7637","65K","LED","16 bit Parallel","6.00"]
["TM128128A4KFWGWC22","1.44","128x128","25.49x26.49","32.36x38.00","ST7637","65K","LED","8 bit Parallel","6.00"]
["TM128128C5KFWGWB-2","1.49","128x128","25.33x28.02","33.30x41.60","UC1697V","65K","LED","8 bit Parallel","6.00"]
["MI128128NK-1","1.50","128x128","26.10x28.15","33.35x41.64","ST7637","65K","LED","16 bit Parallel","6.00"]
["MI128128WK","1.50","128x128","26.10x28.15","33.35x41.64","ST7637","65K","LED","8 bit Parallel","12.00"]
["TM128160E5KFWGWA","1.72","128x160","27.25x34.07","33.54x63.93","ST7669V","65K","LED","8 bit Parallel","6.00"]
["MI128160KK","1.75","128x160","27.25x35.03","34.7x46.7","S6B33BF","65K","LED","CPU,SPI","12.00"]
["MI128160KK-1","1.75","128x160","27.25x35.03","34.7x46.7","S6B33BF","65K","LED","CPU,SPI","12.00"]
["MI128160OK","1.75","128x160","27.254x35.07","34.54x63.93","ST7669V","65K","LED","Parallel","6.00"]
["MI128160PK","1.75","128x160","27.254x35.03","34.7x60","S6B33BLX01-BOC8","65K","LED","Parallel","6.00"]
["MI128160LK","1.92","128x160","30.71x37.99","38.40x52.20","ST7669V","65K","LED","8 - 16 bit Parallel","6.00"]
["MI240160AK-1","2.70","240x160","56.87x36.95","68.68x48.65","ST8016+ST8024","65K","LED","RGB","12.00"]
["MI320240AK","3.50","320x240","67.19x50.39","81.20x67.10","IST3033 + IST3032TA0","65K","LED","RGB","6.00"]
["MI320240EK-1","5.70","320x240","115.19x86.38","154.6X114.8","NT7702 / NT7707","65K","CCFL","Parallel","6.00"]

{"sheet":"EDT","index":12,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Emerging"]
["Display"]
["Technologies"]
["Corp."]
[]
["CSTN"]
["Part Number","Size (inch)","Dots","Module Size (mm) witout PFC","Viewing Area","LCD Type","Color","Controller","Num Pins","Supply (V)","DATA Bus (bit)"]
["ER0120A7NM6-ROHS","1,2\"","128xRGBx96","31x33,4x2,9","26,38x21,93","CSTN Transmissive","65k (8bit)","NT7571",24,"2,7V","8 bit"]
["ER0132A0NM6-ROHS","1,32\"","128xRGBx128","31,15x37x2,7","24,63x25,91","CSTN Negative Transmissive","65k","S6B33BGA01",30,"2,8V","16 bit"]
["ER0137A0NM6-GP","1,37\"","96xRGBx64","39,07x34,1x6,15","30,8x24,59","FSTN Transmissive",null,"UC1693U",20,"2,8V","8 bit"]
["ER015007NM6-ROHS","1,5\"","128xRGBx128","35,6x39,6x3,6","27,3x27,3","CSTN Transmissive","65k (16bit)","ST7637",30,"2,8V","16 bit"]
["ER018001NM6-RoHS","1,8\"","128xRGBx160","36,4x71,6x4,5","30,54x36,04","CSTN Transmissive","65k (16bit)","S6B33BC",40,"3,0V","16 bit"]
["ERA0262A0NMU-ROHS","2,62\"","132xRGBx65","68,5x44,2x5,8","62x33,8","CSTN Transmissive Anti-Glare","65k (16bit)","NT7573",28,"3,0V","16 bit"]
["ER0300A2NM6-ROHS","3,0\"","240x160","87,3x61,2x5,2","63,3x48,7","CSTN Transmissive",null,"No (Common & Segment Driver)",24,"2,5…5,5","4-bit"]
["ER031000NM6-RoHS","3,1\"","240xRGBx240","68,1x68,1x5,25","57x57","CSTN Transmissive",null,"No (Common & Segment Driver)",20,"3,0…3,6","8 bit"]
["ER0350A1NM6-STD","3,5\"","320xRGBx240","84,1x69,8x8,2","75,1x57,3","CSTN Transmissive",null,"No (Common & Segment Driver)",20,"3,0…3,6","8 bit"]
["ER038001NM6-RoHS","3,8\"","320xRGBx240","92x73x4,8","78,8x59,6","CSTN Transmissive",null,"No (Common & Segment Driver)",16,"2,5…5,5","8 bit"]

{"sheet":"DLC","index":13,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Datasheets"]

{"sheet":"KET","index":14,"n_rows":76,"n_cols":13,"rows_kept":76,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["KET","Link"]
["Graphic"]
["Monochrome"]
["P/N","Resolution","Module size (mm)","Viewing Area (mm)","Dot Pitch (mm)","Dot Size (mm)","Duty","Controller","Backlight"]
["G10656A-2 ","106x56 ","36.6x28.0  ","32.6x17.6  ","0.29x0.29 ","0.28x0.27 ","1/65 ","KS0724  ","Y/G LED "," "]
["G12864A1","128x64 ","69.1x50.0 ","66.1x39.0 ","0.475x0.515 ","0.45x0.49 ","1/65 ","NT7532 ","LED "," "]
["G12864B1","128x64 ","64.00x45.00 ","59.00X34.00 ","0.45x0.48 ","0.43x0.46 ","1/65 ","NT7541 ","white LED "," "]
["G12864H-5 ","128x64 ","61.0x38.5 ","52.0x26.5 ","0.38x0.38  ","0.34x0.34 ","1/65 ","ST7565P ","White LED "," "]
["G12864R ","128x64 ","58.0x37.5 ","53.0x27.5 ","0.37x0.37 ","0.34x0.34 ","1/65 ","ST7565R-G ","white LED "," "]
["24064Q ","240x64 ","125.0x60.0 ","111.6x37.0 ","0.44x0.50 ","0.41x0.47 ","1/64 ","SDN8080G-LQFP","Y/G LED "," "]
["160128A-1 ","160x128 ","130.0x102.0 ","101.0x82.0 ","0.58x0.58 ","0.54x0.54 ","1/128 ","T6963C  ","BLUE, white LED"," "]
["240128A-3 ","240x128 ","144.0x104.0 ","114.0x64.0  ","0.45x0.45  ","0.40x0.40  ","1/128 ","T6963C  ","Blue ,White LED  "," "]
["G240128I","240x128 ","93.0x53.0 ","86.15x47.78 ","0.352x0.346 ","0.337x0.331 ","1/128 ","UC1611S ","Blue LED "," "]
["G240160E-1 ","240x160 ","83.8x60.0 ","69.6x47.6 ","0.275x0.275 ","0.26x0.26 ","1/160 ","ST7586S ","white LED "," "]
["320240I-1 ","320x240 ","160.0x109.0 ","119.8x90.6 ","0.36x0.36  ","0.33x0.33  ","1/240 ","S1D13700 ","White LED  "," "]
[]
[]
["TFT"]
["P/N","Size (inch)","Dot Format","Active Area (mm)","Outline Size (mm)","Backlight","Top.(°C)","T storage (°C)","Interface","Colors","Remarks"]
["T220220A0138 ","1.38 ","220xRGBx220 ","35.1x35.1","42.4x46.9 ","  LED","-20-70 ","-30-80 ","16 bit parellel "," ","Circle "]
["T128160G0177-1 ","1.77 ","128xRGBx160 ","28.03x35.04  ","34.7x47.0 ","  1LED","-20-70 ","-30-80 ","SPI ","65K/262K "]
["T176220I0200","2.0 ","176xRGBx220 ","31.68x39.60 ","38.03x51.65 ","  3LED","-20-60 ","-30-70 ","CPU 8/16bit ","65/262K ","With TP "]
["T240320E0220-1 ","2.2 ","240xRGBx320 ","33.84x45.12 ","40.6x56.6 ","  4LED","-20-70 ","-30-80 ","RGB 18bit+3SPI ","262K "]
["T240320W0220 ","2.2 ","240xRGBx320 ","33.48x44.46 ","40.54x56.46 ","  3LED","-20-70 ","-30-80 ","RGB ","262K "]
["T320240A0230-1","2.3 ","320xRGBx240 ","46.75x35.06 ","51.0x45.8 ","  4LED","-20-70 ","-30-80 ","16 bit parellel ","65/262k ","With TP "]
["T320240A0230","2.3 ","320xRGBx240 ","46.75x35.06 ","51.0x45.8 ","  4LED","-20-70 ","-30-80 ","16 bit parellel ","65/262k "]
["T240320L0240-3","2.4 ","240xRGBx320 ","36.72x48.96 ","42.72x60.26 ","  4LED","-10-60 ","-20-70 ","CPU16bit/8bit bus ","262K ","With TP "]
["T240320R0240-1 ","2.4 ","240xRGBx320 ","36.72x48.96 ","42.72x60.26 ","  4LED","-20-70 ","-30-80 ","8/9/16/18bit Parellel ","262K/65K "]
["T240320R0240-2 ","2.4 ","240xRGBx320 ","36.72x48.96 ","42.72x60.26 ","  4LED","-10-60 ","-20-70 ","RGB ","262K ","With TP "]
["T240320S0240-2 ","2.4 ","240xRGBx320 ","36.72x48.96 ","42.72x60.26 ","  4LED","-20-70 ","-30-80 ","CPU ","262K "," "]
["T240320S0240-3 ","2.4 ","240xRGBx320 ","36.72x48.96 ","42.72x60.26 ","  4LED","-20-70 ","-30-80 ","CPU ","262K ","With TP "]
["T240320S0240-4 ","2.4 ","240xRGBx320 ","36.72x48.96 ","42.72x60.26 ","  4LED","-20-70 ","-30-80 ","CPU ","262K "," "]
["T240320S0240-5 ","2.4 ","240xRGBx320 ","36.72x48.96 ","42.72x60.26 ","  4LED","-20-70 ","-30-80 ","CPU ","262K ","With TP "]
["T320240V0240-2 ","2.4 ","320xRGBx240 ","48.0x36.0 ","53.0x46.42 ","  4LED","-20-70 ","-30-80 ","CPU/SPI/RGB ","262K "," "]
["T240400Q0283-3 ","2.83 ","240xRGBx320 ","43.2x57.6 ","50.2x69.3 ","  4LED","-20-70 ","-30-80 ","18bit p 18bit RGB+SPI ","262K "," "]
["T240400S0283","2.83 ","240xRGBx320 ","47.0x60.1 ","50.0x69.2 ","  4LED","-20-70 ","-30-80 ","8/9/16/18bit Parellel ","262K/65K ","Transflective "]
["T240320E0320-3 ","3.2 ","240xRGBx320 ","48.6x64.8 ","57.54x79.2 ","  5LED","-10-60 ","-20-70 ","CPU/RGB/Serail ","262K ","With TP "]
["T240320H0320-1 ","3.2 ","240xRGBx320 ","48.6x64.80 ","57.54x79.02 ","  5LED","-10-60 ","-20-70 ","System parallel/RGB ","262K ","Transflective With TP "]
["T240320H0320","3.2 ","240xRGBx320 ","48.6x64.8 ","57.54x79.2 ","  5LED","-20-70 ","-30-80 ","System parallel/RGB ","262K ","Transflective "]
["T480272H0430-2 ","4.3 ","480xRGBx272 ","95.04x53.856 ","105.5x67.2 ","  LED","-20-70 ","-30-80 ","24bit RGB ","16.7M ","With TP "]
["T480272H0430-3 ","4.3 ","480xRGBx272 ","95.04x53.856 ","105.5x67.20 ","  LED","-20-70 ","-30-80 ","24bit RGB ","16.7M "," "]
["T480272K0430-1 ","4.3 ","480xRGBx272 ","95.04x53.86 ","105.5x67.2 ","  10LED","-20-70 ","-30-80 ","24bit RGB ","16.7M "," "]
["T480272A0470-1 ","4.7 ","480xRGBx272 ","103.68x58.75 ","114.24x72.88 ","  11LED","-20-60 ","-30-70 ","24bit RGB+SPI ","16.7M "," "]
["T480272A0470-3 ","4.7 ","480xRGBx272 ","103.68x58.752 ","114.3x72.5 ","  10LED","-20-60 ","-30-70 ","RGB 24bit with TCON ","16.7M ","with TP "]
["T480272A0470-4 ","4.7 ","480xRGBx272 ","103.68x58.752 ","114.3x72.5 ","  10LED","-20-60 ","-30-70 ","24bit RGB ","16.7M "," "]
["T800480B0500 ","5.0 ","800xRGBx480 ","108.0x64.8 ","120.7x76.3 ","  LED","-20-70 ","-30-80 ","24bit RGB ","16.7M "," "]
["T640480H0500 ","5.0 ","640xRGBx480 ","101.57x76.18 ","117.65x88.43 ","  18LED","-20-70 ","-30-80 ","24bit RGB ","16.7M "," "]
["T480272L0500-1 ","5.0 ","480xRGBx272 ","110.88x62.832 ","120.7x75.8 ","  LED","-20-70 ","-30-80 ","24bit RGB ","16.7M "," "]
["T800480M0500 ","5.0 ","800xRGBx480 ","108.0x64.8 ","118.5x77.55 ","  14LED","-20-70 ","-30-80 ","24bit RGB ","262K ","With TP "]
["T640480BA0570","5.7 ","640xRGBx480 ","115.2x86.4 ","144.0x104.6 ","  21LED","-30-85 ","-30-85 ","18bit RGB ","262k "," "]
["T640480E0570-2 ","5.7 ","640xRGBx480 ","127.0x98.43 ","115.2x86.4 ","  21LED","-20-70 ","-30-80 ","18bit RGB ","262K ","with TP "]
["T640480E0570-5 ","5.7 ","640xRGBx480 ","115.2x86.4 ","127.0X98.43 ","  21LED","-20-70 ","-30-80 ","18bit RGB ","262K "," "]
["T640480K0570-1 ","5.7 ","640XRGBX480 ","115.2x86.4 ","127.0x98.43 ","  21LED","-20-70 ","-30-80 ","18bit RGB ","262K ","with TP "]
["T640480K0570 ","5.7 ","640xRGBx480 ","115.2x86.4 ","127.0x98.43 ","  21LED","-20-70 ","-30-80 ","18bit RGB ","262K "," "]
["T320240P0570 ","5.7 ","320xRGBx240 ","115.2X86.4 ","140.0X104.6 ","  15LED","-30-85 ","-30-85 ","18bit RGB ","262k "," "]
["T800480A0600 ","6.0 ","800xRGBx480 ","133.2X73.8 ","145.5x87.8 ","  21LED","-20-70 ","-30-80 ","24bitRGB ","16.7M "," "]
["T480234GA0700","7.0 ","480XRGBX234 ","154.08X86.58 ","164.9x100.0 ","  LED","-20-70 ","-30-80 ","RGB Vertical stripe ","262k "," "]
["T800480JA0700-1 ","7.0 ","800xRGBx480 ","152.4x91.44 ","165.0x104.44 ","  24LED","-10-60 ","-30-70 ","18bit RGB ","262K ","WithTP "]
["T800480JA0700-2 ","7.0 ","800xRGBx480 ","152.4x91.44 ","165.0x104.0 ","  24LED","-20-70 ","-30-80 ","18bit RGB ","262K "," "]
["T800480JA0700-3 ","7.0 ","800xRGBx480 ","152.4x91.44 ","165.0x104.0 ","  24LED","-20-70 ","-30-80 ","18bit RGB ","262K "," "]
["T800480SA0700","7.0 ","800xRGBx480 ","154.08x85.92 ","164.9x100.0 ","  24LED","-20-70 ","-30-80 ","24bit RGB ","16M ","With TP;With TCON "]
["T800480S0700-3 ","7.0 ","800xRGBx480 ","154.08x85.92 ","164.9x100 ","  LED","-10-60 ","-20-70 ","24bit RGB ","16.7M ","With TP "]
["T800480S0700","7.0 ","800xRGBx480 ","154.08x85.92 ","164.9x100 ","  LED","-20-70 ","-30-70 ","24bit RGB ","16.7M "," "]
["T800600F0800 ","8.0 ","800xRGBx600 ","162.0x121.5 ","183.0x141.0 ","  27LED","-20-70 ","-30-80 ","18/24bit RGB ","16.7M "," "]
["T800600J1040-1 ","10.4 ","800xRGBx600 ","211.2x158.4 ","236.0x176.9 ","  36LED","-20-70 ","-30-80 ","TTL ","262K "," "]
[]
[]
["OLED"]
["P/N","Size (inch)","Dot Format","A.A. (mm)","Outline Size (mm)","Interface","Colors"]
["O9664F0095-1 ","0.95 ","96x64 ","20.135x13.42 ","24.8x22.42 ","8bit 6800, 8bit 8080 ","65K R/Y/G/B/W ",null,null,null," "," "," "]
["O12832B0200 ","2.0 ","128x32 ","50.535x10.695 ","59.0x18.86 ","8bit parallel, serial ","White ",null,null,null," "," "," "]
["O12864A0270-1 ","2.7 ","128X64 ","61.41x30.69  ","89.7x47.2 ","8BIT parellel 4spi ","Yellow ",null,null,null," "," "," "]
["O12864A0270 ","2.7 ","128x64 ","61.41x30.69  ","75.0x53.5  ","8BIT parellel 4spi ","Yellow,Green ",null,null,null," "," "," "]
["O12864D0154 ","2.7 ","128x64 ","61.41x30.69  ","75.0x53.5 ","8BIT parellel 4spi ","Yellow,Green ",null,null,null," "," "," "]
["O25664B0312","3.12 ","256x64 ","76.78x19.18 ","88.0x27.8 ","8BIT parellel 4spi ","LIGHT BLUE ",null,null,null," "," "," "]
["O25664C0270","2.7 ","256x64 ","66.54x16.62 ","82.0x25.5 ","8BIT parellel 4spi ","R/Y/G/B/W ",null,null,null," "," "," "]

{"sheet":"Repro","index":15,"n_rows":40,"n_cols":12,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Sharp","Reproele.jp"]
["Offer811.mht","Repro Electronics Corporation"]
["Product Number","aka Module name","Size (inch)","Type","Resolution (pixel)","Colors","Controller","Data bits","Interface","Pins","Connector Maker","P/N Connector"]
["151AB00",null,"1,8\"","STN","120x160",65.536,{"$nulls":4},"Shin-Etsu Polymer Co. Ltd","Customer"]
["153CB00",null,"1,8\"","TFT","132x176",65.536,{"$nulls":4},"Matsushita Electric Works","AXK 72 8147BK1"]
["161AA00",null,"1,9\"","STN","120x160",4.096,{"$nulls":4},"JAE","IL-FHJ-33S-HF-N1"]
["162BA00",null,"1,9\"","TFD","132x162",4.096,{"$nulls":4},"Shin-Etsu Polymer Co. Ltd","Customer"]
["163CB00",null,"1,9\"","TFT","132x176",65.536,{"$nulls":4},"JAE","WA5B070VA2E3000"]
["163CB01",null,"1,9\"","TFT","132x176",65.536,{"$nulls":4},"JAE","WA5B070VA2E3000 "]
["163CB02",null,"1,9\"","TFT","132x176",65.536,{"$nulls":4},"JAE","WA5B070VA2E3000"]
["163CB03",null,"1,9\"","TFT","132x176",65.536,{"$nulls":4},"Matsushita Electric Works","AXK 72 8147BK1"]
["163FB00",null,"1,9\"","TFT","160x216",65.536,{"$nulls":4},"JAE","WA5B070VA2E3000"]
["172BA00",null,"2,0\"","TFD","132x162",4.096,null,"8","conn",20,"Matsushita Electric Works","AXK 5F 2034BK1"]
["173AA00",null,"2,0\"","TFT","120x160",4.096,{"$nulls":4},"JAE","FB6S033JA1R3000"]
["182AA00",null,"2,1\"","TFD","120x160",4.096,{"$nulls":4},"JAE","FB6S021JA1R3000"]
["182CC00",null,"2,1\"","TFD","132x176",262.144,{"$nulls":4},"Matsushita Electric Works","AXK 5F 3034BK1"]
["182CC01",null,"2,1\"","TFD","132x176",262.144,"Maybe S1D15G10","16/8","Conn",30,"Matsushita Electric Works","AXK 5F 3034BK1"]
["182CC02",null,"2,1\"","TFD","132x176",262.144,{"$nulls":4},"Matsushita Electric Works","AXK 5F 3054BK1"]
["183CB00",null,"2,1\"","TFT","132x176",65.536,{"$nulls":4},"Matsushita Electric Works","AXK746127BK1"]
["183CB01",null,"2,1\"","TFT","132x176",65.536,{"$nulls":4},"Molex","54765-2476"]
[]
["183DB00",null,"2,1\"","TFT","160ｘ160",65.536,{"$nulls":4},"JAE 15 pins","FF0215SS1-R3000"]
["192GC00",null,null,null,"240x320"]
["193CB00"]
["193FB00",null,null,null,"160x216"]
["193GB00"]
["193GB01"]
["193GC00",null,null,null,"240x320"]
["1B3GB02"]
["1B3GC01"]
["1B3GC02"]
["1B3GC03"]
["1B3MC00"]
["1B3MC01"]
["1G3LC00"]
[]
[]
[]
["RXTMK2V250"]
["RXTMK2V300"]

{"sheet":"Mairong","index":16,"n_rows":15,"n_cols":9,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"CSTN LCM List"]
[]
["Size","Number of Dots","Model No.","Outline Dimension (W x H x T) mm","View area V/A (W x H) mm","Active area A/A (W x H) mm","Color","IC","Driving Method (Duty)"]
["1.1\"","96(RGB)*96","MRGG090907-6TCNNA","25.81*34.01*1.2","20.92*20.4","18.71*18.71","65K","S6B33B5A","1/96"]
["1.47\"","128(RGB)*128","MRGG121217-6TCLWA","34.7*55*3.3","29.17*29.17","26.099*26.865","65K","S6B33B6","1/132"]
["1,47\"","128(RGB)*128","MRGG121217-6TCLWC","34.7*55*3.3","29.17*29.17","26.099*26.865","65K","S6B33B6","1/132"]
["1.47\"","128(RGB)*128","MRGG121217-6TCLWE","34.7*61.05*3.3","29.17*29.17","26.099*26.865","65K","S6B33B6","1/132"]
["1.47\"","128(RGB)*128","MRGG121217-6TCLWF","34.7*61.05*3.3","29.17*29.17","26.099*26.865","65K","S6B33B6","1/132"]
["1.51\"","128(RGB)*128","MRGG121227-7TCLWA","33.35*49.44*3.75","28.3*30.17","26.1*28.15","65K","S6B33B6","1/132"]
["1.51\"","128(RGB)*128","MRGG121227-7TCLWB","33.35*52.1*3.75","28.3*30.17","26.1*28.15","65K","S6B33B6","1/132"]
["1,51\"","128(RGB)*128","MRGG121227-7TCLWE","33.35*52.1*3.75","28.3*30.17","26.1*28.15","65K","S6B33B6","1/132"]
["1,47\"","128(RGB)*128","MRGG121228-6TCLWA","34*54.7*3.3","29.3*29.9","26.1*26.868","65K","S6B33BG","1/132"]
["1.47\"","128(RGB)*128","MRGG121231-7TCLWB","35.2*50.7*2.85","29.3*29.9","26.1*26.868","65K","S6B33BG","1/132"]
["1.51\"","128(RGB)*128","MRGG121236-7TCLWA","33.35*52.1*3.75","28.3*30.17","26.1*28.15","65K","S6B33BG","1/132"]
["1.51\"","128(RGB)*128","MRGG121238-7TCLWA","33.35*52.1*3.75","28.3*30.17","26.1*28.15","65K","ST7637","1/132"]

{"sheet":"CSTN","index":17,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["IST3032"]
["IST3033"]
["S6B3301","Samsung"]
["S6B33BF","Samsung","132x162","65k","Color STN"]
["ST7637","Sitronix","132x132","65k"]
["ST7687S","Sitronix","128x128","65k"]
["ST7689","Sitronix","128x160","65k"]
[]
["UC1681","Ultrachip","68x98",null,"C-STN"]
["UC1697","Ultrachip","128x128",null,"C-STN"]
["UC1698","Ultrachip","160x128",null,"C-STN"]
[]
[]
[]
[]
[]
["HD66791","Renesas","128x160","64k/262",null,"Parallel I/O","COG"]
["S1D15G17E","Epson","128x128","65k",null,"Parallel I/O","COG"]
["S6B33B0A","Samsung","128x128","65k",null,"Parallel I/O","COG"]
["S1D15G27","Epson","128x128","65k",null,"Parallel I/O","COG"]
["L1F10289","Epson","96x64","65k",null,"Parallel I/O","COG"]
["ST7565",null,"64x48","Mono",null,"Serial Interface","COG"]
["SH1101A","RITDISPLAY","96x64","OLED",null,"Serial Interface","COG"]
["S6D0123","Samsung","128x160","Color",null,"Parallel I/O","COG"]

{"sheet":"TFT","index":18,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["HX8328-A","Himax"]
["S6D04H0","Samsung"]
["LDS285","Leadis","240x320"]
["SSD1289","Solomon"]
["HX8347-A","Himax","240x320",null,"TFT"]
["S6D0154","Samsung","240x320","262k","TFT"]
["R61505W","Renesas","240x320","262k","TFT"]
["HX8655-A","Himax"]
["HX8218-C01","Himax"]
["R61580","Renesas","240x320","262k","TFT"]
["HX8369-A","Himax","480x864","16,7M","TFT"]
["HX8250-A01","Himax"]
["HX8352-C(T)","Himax","240x432","262k","TFT"]
["HX8615B","Himax"]
["HX8678-A","Himax"]
["S6D04D1X21","Samsung"]
["HX8353-C","Himax","132x162","262k","TFT"]
["HX8363-A","Himax","480x864","16,7M","TFT"]
["R61581","Renesas","320x480","262k","TFT"]
["HX8368-A (N)","Himax","320x240","262k","TFT"]
["HX8262-A","Himax"]
["SSD2215","Solomon"]
["S6D05A0","Samsung"]
["LGDP4531"]
["NT35582","Novatek"]
["S1D19122","Seiko Epson"]
["HX8662-C","Himax"]
["LG4573"]
["ILI9331"]
["ILI9326"]
["RM68040"]
["ILI9481"]
["NT39406","Novatek"]
["LDS291","Leadis","480x640","262k","TFT"]
["R61526","Renesas","240x320","262k","TFT"]
["R61509","Renesas","240x432","262k","TFT"]
["HX8232-B","Himax"]
["SSD2128","Solomon"]
["S6D0164X01","Samsung"]
["NT39327","Novatek"]
["HX8258-A","Himax"]
["HX8677-A","Himax"]
["HX8268-A","Himax","480x480"]
["HX8357-B","Himax","320x480","262k","TFT"]
["NT39407S","Novatek"]

{"sheet":"Monochrome","index":19,"n_rows":5,"n_cols":5,"rows_kept":5,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["NT7702","Novatek"]
["NT7701","Novatek"]
["UC1610","Ultrachip","128x160","4S","STN"]
["NT7538","Novatek"]
["UC1698u","Ultrachip"]

{"sheet":"STE_ICs","index":20,"n_rows":11,"n_cols":2,"rows_kept":11,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
["STE9668DIE2/A-3","STE6596DIE-2(DICE,PBF) D/C04"]
["STE9668DIE2/B-1","STE6596DIE2"]
["STE9668DIE2/D","STE6596DIE-2"]
["STE9668DIE2/C","STE6596DIE2(PBF) D/C04"]
[]
["STE9668D2D/A-3"]
["STE9668D2D/B-1"]
["STE9668D2D/C"]
["STE9668D2D/D"]

{"sheet":"Leadis_ICs","index":21,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["LeadisTechnology Inc."]
[]
["Technology","Product","Resolution","Colors"]
["Mono STN","LDS162","96 x 68","Monochrome"]
["Color STN","LDS176","132 RGB x 132","4K"]
[null,"LDS184(A)","98 RGB x 70","65K"]
[null,"LDS181","101 RGB x 80","65K"]
[null,"LDS183","128 RGB x 128","65K"]
[null,"LDS186","128 RGB x 160","65K"]
[null,"LDS191","132 RGB x 162","262K"]
[null,"LDS192","132 RGB x 162","262K"]
["TFT","LDS273","132 RGB x 162","262K"]
[null,"LDS274","176 RGB x 240","262K"]
[null,"LDS279","128 RGB x 160, 120 RGB x 160, 128 RGB x 128","262K"]
["LTPS TFT","LDS314","176 RGB x 220, 240 RGB x 320","262K"]
[null,"LDS321","288 RGB x 352, 320 RGB x 480","262K"]
[null,"LDS331","132 RGB x 162, 128 RGB x 160, 130 RGB x 130","262K"]

{"sheet":"IST_ICs","index":22,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Model","Features","Compatible Models","A type","Working voltage"]
["IST7101","240 Com./Seg. Driver 2Bit/4Bit ",null,"COG","2.5V-5.5V"]
["IST7001 ","240*96 Single Chip Driver ","UC1608 ","COG","2.4~3.6V"]
["IST3753","168*132(4GS) Single Chip Drive ",null,"COG","2.4~3.6V"]
["IST3168","128*128(4GS) Single Chip Driver ","HD66750S/SSD1852/UC1607i","TCP/COG ","1.8-3.6V"]
["IST3104","132RGB*132 true 65K color Single Chip Driver ","S6B33B0A/PCF8833/HD66766/SSD1781/UC1687I","COG"]
["IST3103","104RGB*84 true 65K color Single Chip Driver ","HD66768/SSD1773/UC1682i","COG"]
["IST3101","104RGB*84 4K color Single Chip Driver ","HD66768/SSD1770/UC1612i","COG","1.7-3.6V"]
["IST3033","Hi-fas 320 Seg. Driver","HD66130/SPLC563C/ST8624 ","COG","2.5V-5.5V"]
["IST3032 ","Hi-fas 240 Com. Driver","HD66137/SPLC564C/ST8601/IT7020 ","TCP/COG","2.5V-5.5V"]
["IST3031","Hi-fas 320 Seg. Driver ","HD66130/SPLC563C/ST8624/IT7012 ","TCP","2.5V-5.5V"]
["IST3029","240 Channel Seg. Driver ","LH1548F/EK7103 ","TCP","2.5V-5.5V"]
["IST3028","120 Channel Com. Driver","LH1530F/EK7102 ","TCP","2.5V-5.5V "]
["IST3025 ","160 Com./Seg. Driver","LH1560/NT7701/NT7705//EM65160/ST8016 ","TCP/COG ","2.5V-5.5V "]
["IST3017","240*96 Single Chip Driver ",null,"COG","2.4-3.6V "]
["IST3015","132*65 Single Chip Driver ","KS0724/NT7502/ST1565/SSD1815/UC1606 ","TCP","2.4-3.6V "]

{"sheet":"Samsung_ICs","index":23,"n_rows":128,"n_cols":4,"rows_kept":128,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Samsung","DISPLAY      DRIVE      IC"]
["MFAM ","Device","Function","PKG"]
["Color","S6B33B0","144*176:65K","COG"]
["Color","S6B33B2","132*162:65K","COG"]
["Color","S6B33B2","132*162:65K-COF","TCP"]
["Color","S6B33B3","133*132:65K","COG"]
["Color","S6B33B5","96*96:65K","COG"]
["Color","S6B33BK","96*96:65K","COG"]
["Color","S6B33B6","132*132:65K","COG"]
["Color","S6B33BGA01-BPCY","132*132:65K","COG"]
["Color","S6B33B1","132*132:65K","COG"]
["Color","S6B33B1","132*132:65K","TCP"]
["Color","S6B33B9","132*162:65K::pallet:shrink of S6B33B2","COG"]
["Color","S6B33BC","132*162:65K:","COG"]
["Color","S6B33BFX01-BOCY","132*162:65K:","COG"]
["Color","S6B33BL","132*162:65K:","COG"]
["Color","S6B33BJ","132*162:65K:","COG"]
["Color","S6B33BAX01-BAFY","132*132:65Kpallet:For Nokia","COG"]
["Color","S6B33BAX11-B1DK","132*132:65Kpallet:For Nokia","COG"]
["Color","S6B33BEX01-BOFY","132*132:65Kpallet:For Nokia","COG"]
["Color","S6B33BG","128*128:65K","COG"]
["Color","S6B3301","128*128:65K","COG"]
["Color","S6B3306","128*128:65K","COG"]
["Color","S6B33BDX01-BAFY","98*70:65K:For Nokia","COG"]
["Color","S6B33BDX11-B1DK","98*70:65K:For Nokia","COG"]
["Color","S6B33D1X01-BOFK","128*160:260K:For Nokia","COG"]
["Color","S6B33D2","128*160:260K:For Nokia","COG"]
["Color","S6B33D3","96*128:260K:For Nokia","COG"]
["Color","S6B33D4","128*160:260K:For Nokia","COG"]
["Color","S6B33C1X01-BOCY","96RGB seg*66com, 4K Color 1Chip","COG"]
["MTFT","S6D1201X01-BOCI","360/324 ch Source Driver for PDA","COG"]
["MTFT","S6DG101X01-BOCI","320/322 ch Gate Driver for PDA","COG"]
["MTFT","S6DO110A31-BOCY ","132RGB*176ch  65K TFT 1chuip(Source+Gate+Power)","COG"]
["MTFT","S6D0114X01-BOCY","132RGB*176ch  65K TFT 1chuip(Source+Gate+Power),RGB I/F","COG"]
["MTFT","S6D0115","176*240(Qcif+)Gateless:65K/260K:CPU/RGB 1/F","COG"]
["MTFT","S6D0117A11-BOCX","132*132(Sub):64k260k:Low Power","COG"]
["MTFT","S6D0118A01-BOCX","176*240(Qcif +):260k","COG"]
["MTFT","S6D0118A01-BJDX","176*240(Qcif +):260k","COG"]
["MTFT","S6D0119X01-BHCE","176*240(Qcif +):260k:Gateless&Memoryless","COG"]
["MTFT","S6D0120","Dyal(240*320)+(128*160):260k:Gateless&Memoryless","COG"]
["MTFT","S6D0123","132*176(Qcif ):65k/260k:CPU/RGB 1/F","COG"]
["MTFT","S6D0128","176*240(Qcif+):260k:Shrink of S6D0118","COG"]
["MTFT","S6D0129X11-BOCY","240*320(Qvga):260K:All in one chip ","COG"]
["MTFT","S6D0139X11-BOCY","240*320(Qvga):260K:All in one chip ","COG"]
["MTFT","S6D0133","128*160(qqVGA):65K:Only for AMLCD","COG"]
["MTFT","S6D0134","128*160(qqVGA):65K:Minor Change","COG"]
["MTFT","S6D0136X02-BOFK","130*130:65k:For Nokia","COG"]
["MTFT","S6D0137X01-BOFK","132*162:65k:For Nokia","COG"]
["MTFT","S6D0138","240*320(Qvga):16M:For Nokia","COG"]
["MTFT","S6D0140","240*320(Qvga):260K:For Optrex","COG"]
["MTFT","S6D0142","240*320(Qvga):260K:MD01","COG"]
["MTFT","S6D0144","128*160(qqVGA):260K","COG"]
["MTFT","S6D0147","132*162&128*160:260K:For Nokia","COG"]
["MTFT","S6D0149","240*320(Qvga):16M:For Nokia","COG"]
["MTFT","S6D0154","240*320(Qvga):260k","COG"]
["MTFT","S6D0151","128*160(qqVGA):260K","COG"]
["MTFT","S6D0164","176*240(Qcif+):260k:Shrink of S6D0128","COG"]
["MTFT","S6D03B0","176*240(Qcif+):260k:Shrink of S6D0164","COG"]
["MTFT","S6D0170X01-BOCY","240*432(WQvga):260k","COG"]
["MTFT","S6D0171","240*320(Qvga):16M","COG"]
["MTFT","S6D0206","240*320(Qvga):260k:Gateless&Memoryless","COG"]
["MTFT","S6D2115","176*240(Qcif+):shrink of S6D0115","COG"]
["MTFT","S6D2101","240*320(Qvga)","COG"]
["MTFT","S6D2105","240*320(Qvga)","COG"]
["MTFT","S6D1120","240*320(Qvga):260k(18bit) for NOKIA","COG"]
["MTFT","S6D1121","240*320(Qvga):260k(18bit)","COG"]
["MTFT","S6D1142","240*320(Qvga):260k(18bit) for NOKIA","COG"]
["MTFT","S6D2121","320*240(L-Gvga):260K","COG"]
["MTFT","S6D1144","240*320(Qvga):16M(24bit)","COG"]
["MTFT","S6D1202","240*320(Qvga):16M(24bit)","COG"]
["MTFT","S6D2204","480*640(VGA):260K:4Color Rendering","COG"]
["MTFT","S6D2229","176*220(Qcif+):260K","COG"]
["MTFT","S6D0626A01-BOCI","240 ch. Source Driver","COG"]
["MTFT","S6D0628X01-WOXC","240 ch. Source Driver","COG"]
["MTFT","S6D06A0","480*640 VGA:16M","COG"]
["MTFT","S6D05A0","320*480 Hvga:16M","COG"]
["MTFT","S6D05A1","320*480 Hvga:16M","COG"]
["MTFT","S6D04D0","240*432 WqVGA","COG"]
["MTFT","S6D04D1","240*432 WqVGA","COG"]
["MTFT","S6D04D3","240*432 WqVGA","COG"]
["MTFT","S6D04M0","240*320 qVGA:16M","COG"]
["MTFT","S6D04E0","240*320 qVGA:16M","COG"]
["MTFT","S6D04E1","240*320 qVGA:16M","COG"]
["MTFT","S6D04E2","240*320 qVGA:16M","COG"]
["MTFT","S6D04P0","240*320 qVGA:260K","COG"]
["MTFT","S6D04H0","240*320 qVGA:260K","COG"]
["MTFT","S6D04H1","240*320 qVGA:260K","COG"]
["MTFT","S6D02A1","128*160 qqVGA:260K","COG"]
["MTFT","S6D02A2","128*160 qqVGA:260K","COG"]
["MTFT","S6D2223","240*432 WqVGA:16M","COG"]
["MTFT","S6D24D0","240*432 WqVGA:16M","COG"]
["MTFT","S6D2213","240*320 Qvga:16M","COG"]
["MTFT","S6D24B0","240*320 Qvga:16M","COG"]
["MTFT","S6D24B1","240*320 Qvga:16M","COG"]
["MTFT","S6D24A0","240*320 Qvga  260k","COG"]
["MTFT","S6D24A1","240*320 Qvga  260k","COG"]
["MTFT","S6D24A2","240*320 Qvga  260k","COG"]
["MTFT","S6D16A0","480*864 P-WVGA:16M","COG"]
["MTFT","S6D16A1","480*864 P-WVGA:16M","COG"]
["MTFT","S6D16B0","480*864 P-WVGA:16M","COG"]
["MTFT","S6D16D0","864*480 L-WVGA: 16M","COG"]
["MTFT","S6D16C0","864*480 L-WVGA: 16M","COG"]
["MTFT","S6D16C1","864*480 L-WVGA: 16M","COG"]
["MTFT","S6D16E0","640*480 VGA/NHD","COG"]
["MTFT","S6D66B0","640*480 VGA/NHD","COG"]
["MTFT","S6D15B0","320*480 Hvga:16M","COG"]
["MTFT","S6D14E0","240*432 WqVGA","COG"]
["MTFT","S6D1130","240*320 Qvga 16M","COG"]
["MTFT","S6D14A0","240*320 Qvga 16M","COG"]
["MTFT","S6D14C3","240*320 Qvga 16M","COG"]
["OLED","S6E63M0","480*864 WVGA 16M","COG"]
["OLED","S6E63L0","480*640 VGA:16M","COG"]
["OLED","S6E63J0","640*360 Nhd  16M","COG"]
["OLED","S6E63H0","320*480 Hvga:16M","COG"]
["OLED","S6E63H1","320*480 Hvga:16M","COG"]
["OLED","S6E63D4","240*432 WqVGA 16M","COG"]
["OLED","S6E63G0","240*432 WqVGA 16M","COG"]
["OLED","S6E63G2","240*432 WqVGA 16M","COG"]
["OLED","S6E63F0","240*320 Qvga  16M","COG"]
["OLED","S6E63F6","240*320 Qvga  16M","COG"]
["OLED","S6E63F7","240*320 Qvga  16M","COG"]
["OLED","S6E63D3","240*320 Qvga  260K","COG"]
["OLED","S6E63D2","240*320 Qvga  260K","COG"]
["OLED","S6E13B1","96*96 :65K:PMOLED","TCP"]
["OLED","S6E13C0X-??XN","OLED 256 Color 1 chip (96*64)","TCP"]
["OLED","S6E13D0","96*96:260K:PMOLED","COG"]
["OLED","S6E63D0","176*240(Qcif+):AMOLED","COG"]
["OLED","S6E63D2","240*320(qVGA+):AMOLED","COG"]

{"sheet":"Driver_IC","index":24,"n_rows":74,"n_cols":8,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["KS0107B","Samsung",null,null,null,"Samsung"]
["ST7565R","Sitronix","65x132",null,null,"S6B1713","65 com / 132 seg","STN"]
["ILI9325","ILITEK",null,null,null,"S6B0723","132 seg / 65 com","STN"]
["S6E63D6","Samsung",null,null,null,"KS0715","33 com / 100 seg","STN"]
["HX8347-A01","Himax","240x320","262k","TFT","KS0713","65 com / 132 seg","STN"]
["SH1101A",null,"132x64",null,"OLED/PLED","S6B0741","128 seg / 129 com","STN 4 grayscale"]
["ST7066","Sitronix",null,null,null,"KS0759","81 com / 128 seg","STN"]
["SSD1327","Solomon",null,null,null,"S6B0755","128 seg / 65 com","STN"]
["µPD7225",{"$nulls":4},"S6B0724","132 seg / 65 com","STN"]
["LGDP4532",null,"720-channel","262k",null,"S6B0721","132 seg / 65 com","STN"]
["NT7086","Neotec",null,null,null,"S6B3301","132 RGB x 132","color"]
["SED1335","Epson",null,null,null,"KS0107"]
["HT1621",{"$nulls":4},"KS0108"]
["ILI9320","ILITEK"]
["ILI9340","ILITEK"]
["T6963C","Toshiba"]
["NT7450","Neotec"]
["KS0108B","Samsung"]
["SSD1305","Solomon"]
["SSD1926","Solomon"]
["S6B33B2","Samsung","132x162","65k","Color STN"]
["S1D13705","Epson"]
["ILI9163","ILITEK"]
["NT7534"]
["ILI9328","ILITEK"]
["UC1682","Ultrachip","80x104",null,"Color STN"]
["HX8238-A","Himax","960x240",null,"TFT"]
["SSD1331","Solomon"]
["PT6608","Princeton "]
["ILI9327","ILITEK"]
["ST7921","Sitronix","96 channel"]
["KS0086","Samsung"]
["ST7687S",null,"128x128","65k"]
["R61509V",null,"240x432","260k"]
["ST7565S","Sitronix","65x132"]
["SSD1805","Solomon"]
["SA3086",null,"80channel"]
["ST7549T","Sitronix","68x102"]
["SSD1815","Solomon"]
["ST7522","Sitronix","17x96"]
["S6D0154","Samsung"]
["SSD1322","Solomon"]
["SSD1308","Solomon"]
["LG4525B","LG","528 channel","262k","TFT"]
["NT7532",null,"132x65",null,"STN"]
["NJU6452A"]
["KS0066U","Samsung","16COM / 40SEG"]
["SSD1353","Solomon"]
["HX8655-A"]
["KS0070B","Samsung","16COM / 80SEG"]
["MC2TA7402","MagnaChip",null,null,"TFT"]
["PT6607","Princeton "]
["HX8340",null,"176x220","262k","TFT"]
["FGD0801",null,"128x160","262k","TFT"]
["S6D04H0","Samsung"]
["HT1623","Holtek"]
["UC1681S","Ultrachip","68x98",null,"C-STN"]
["SED1561","S-MOS Systems"]
["ST7732","Sitronix",null,"262k","TFT"]
["S6B0724","Samsung","132 SEG / 65 COM",null,"STN"]
["HX8347-D",null,"240x320","262k","TFT"]
["SSD1303","Solomon"]
["HT16220","Holtek"]
["NT7651",null,"16Cx2 characters + 160 icons"]
["KS0724","Samsung","65 COM / 132 SEG"]
["TLS8103","Teralane ","132x132","65k"]
["ST7773","Sitronix",null,"262k","TFT"]
["TR7707",null,"320x240","16 grayscale","STN"]
["S6B0086","Samsung","80 channel driver"]
["SSD1800","Solomon"]
["HX8345",null,"128x160","262k","TFT"]
["S6A0073","Samsung","34COM/60SEG"]
["S6B33B3A","Samsung","132x132","65k","Color STN"]
["ST7920","Sitronix"]

{"sheet":"Sources","index":25,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["LCM data & sources"]
["pudn"]

{"sheet":"LCD_Types","index":26,"n_rows":37,"n_cols":4,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Handset #","LCD P/N","Glass"]
[]
["NOKIA","ADBB001","IF118FBN1A","LTP700WV-F01"]
["Pantech PN-315",null,"IF283DBN1A","LTE480WQ-F01"]
["SGH-T319","UC120R210A","IM350RB1A","LMS430HF02"]
[null,"UF12R051A","IM180BAC1B","LTE430WQ0x"]
["SGH-C417/416","UF12R089A","IM180BBN1A","LMS350GF08"]
["SCH-A950","UF17E85A","IMM180B31A","LMS350GF04"]
["(Juke, Verizon)",null,"IM186BSO1A","LTV350QV-F04"]
["Global","UF17E117A","IMM200B31A","LMS283GF0x"]
[null,"UF24U46A","IMM200B41A","LMS250GF03"]
["SGH-D800","UF24U47A","IMM200B43A"]
["SGH-P910","UF24U073A","IM220CBN1A","LH283"]
[null,"UG09M09A","IMM175A31A","LH260WQ01"]
[null,"UG12A72A","IMM180A31A","LH220Q03"]
[null,"UG12A105A","IMM180A32A","LH220Q01"]
[null,"UG12A62A","IMM186S42A","LH200Q02"]
[null,"UG12A190A","IM200CSC2A","LH200Q01"]
["Kyocera E1100","UG12R16B","IMM186A31A","LH190JC1"]
["X7700","UG12R21A","IMM186S41A","LB186Q01A1"]
["SGH-E105","UG12R48A","IM200CSO1A","LB180Q01A1"]
["SGH-X460","UG12R99A","IM200CSC2A"]
["SCH-A850","UG12R155G","IM220CST1A"]
[null,"UG12R156G","IM200CST2A"]
["SPH-A420","UG12R87A","NM260PZ1B"]
[null,"UG12R99A","HVT24QV2"]
["SCH-A725","UG12R119A","HVT20QV4"]
["SPH-A820","UG12R157A"]
["SGH-T209","UG12R209A"]
["SGH-C300","UG12R225A"]
["SCH-A650","UG12R076A"]
["SGH-E330N","UG12R110C"]
["SPH-A840","UG12R155"]
["SPH-A820","UG12R157"]
[null,"UG12R185A"]
["SGH-Z630","UG24U062A"]
["YP-K3(Yepp MP3)","PM12HC002BA"]

{"sheet":"List2","index":27,"n_rows":15,"n_cols":1,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
["Mobile phone Lcd screens for China : "]
["Size:1.1\"-3.5\""]
["Type:CSTN,TFT,LTPS,OLED"]
["Resolution:96*68,128*128,QQVGA(128*160),QCIF(176*220),QVGA(240*320),WQVGA(400*234)"]
["Cell:AUO,LG,CMO,CPT,HYDIS,HANNSTAR,WINTEK,HITACHI,SHARP,TPO,SAMSUNG,TMD,PVI"]
["LCD Driver:"]
["Renesas(R61505,R61503,R61509,R61580,R61508)"]
["LG(LGDP4522,LGDP4524,LGDP4531,LGDP4523,LGDP4532)"]
["Novatek(NT39113,NT39115,NT39106,NT39122,NT39102,NT39116)"]
["Samsung(S6D0128,S6D0139,S6D0144,S6D0150,S6D0154,S6D0158,S6D0165,S6D0164)"]
["Orise(SPFD5408,SPFD5420,SPFD54124,SPFD54126)"]
["Himax(HX8356,HX8347,HX8309,HX8312,HX8310,HX8325，HX8345，HX8346)"]
["Ilitek(ILI9325,ILI9320,ILI9221,ILI9220,ILI9326,ILI9225)"]

{"sheet":"Sharp","index":28,"n_rows":14,"n_cols":1,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Sharp"]
["LS024Q3UX01K,LS024Q8UX02,LS022Q8UX01,LS022Q8UX04,LS024Q8UX05,LS035B7UX013,"]
[" LS035B7UG013,LS032B7LX01,LS018A8GB95,LQ035QIDG01/02,LS020B8UD06,LS020B1DD01D,"]
[" LS025Q1UC01;LS028V7DX01;LS032B7LX01;LS038Y7DX01;LS035B7UX01；LS035B7UG01；"]
[" LQ035Q7DH06；LQ035Q7DB02；LQ024B7UD01；LS026B7LX01；LQ026B7UB01;LQ026B7UB03;"]
[" LS030B7UX01;LS033B3UX01,LQ043T3DX01/02,LMS430HF,LTE430WQ-FOB,LS025Q7UX01 "]
[" LS025Q7UA01 ,LS025Q7UX91 ,LS025Q7UX013,LQ035Q1DG01,LQ5RB49 ,LQ056A3AG01 ,LM6Q401 ,"]
[" LG070T3AG02,LQ070Y3DG01 ,LQ080V3DG01 ,LQ104V1DG51 ,LQ104V1DG52 ,LQ104V1DW01 ,"]
[" LQ110Y3DG01,LQ121S1LG45 ,LQ150X1LCN7 ,LS041Y3DX01S ,LS041Y3LW01 ,LS041YBLX01 ,"]
[" LS040B8DB01,LS040B8DY01A ,LS040B8DY01B ,LS039B8LX01B ,LQ038J7DH53 ,LQ038Q7DB03R "]
[" LS037V3DX01,LS035B7UA01B ,LQ035Q7DH ,LS033T8LX0 ,LS032T8LX0 ,LS030B1DC ,LS030T3DC "]
[" LS030T3DW,LS030T3DX ,LS030T8LX ,LS030Y8PX ,LS025Q7UA ,LS025Q1UC ,LS025B7DH ,"]
[" LS025Q7UX,LS024B7DW ,LS024Q3PX01 ,LS024Q8UX ,LS024V8PX ,LS028B7UX ,LS028B8DX0 "]
[" LS028B8DX0 ,LS028B8PX0 "]

{"sheet":"TD025THEA7","index":29,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Display from Chinese MP4 Zarva PMP MV203","Pins on glass","Designation (lettering on glass)","Pins on the ribbon","Designation on the ribbon"]
["TD025THEA7 (40 pin ribbon)",1,"GRSTB",40,"GRESTB"]
["On the glass backing, the inscription:",2,"SHDB",39,"SHDB"]
["TD025WHEB1",3,"STB"]
["2061 3061 4051",4,"SCEN",38,"SCEN"]
["5602",5,"SCL",37,"SCL"]
["25TB1 (large print)",6,"SDA",36,"SDA"]
[null,7,"DIN7",35,"DIN7"]
[null,8,"DIN6",34,"DIN6"]
[null,9,"DIN5",33,"DIN5"]
[null,10,"DIN4",32,"DIN4"]
[null,11,"DIN3",31,"DIN3"]
["The pinout of the ribbon is the same as TD036THEA3",12,"DIN2",30,"DIN2"]
["The controller is likely TPG051",13,"DIN1",29,"DIN1"]
[null,14,"DIN0",28,"DIN0"]
[null,15,"DCLK",27,"DCLK"]
[null,16,"HD",26,"HD"]
[null,17,"VD",25,"VD"]
[null,18,"VCC",24,"VCC"]
[null,19,"GND",23,"GND"]
[null,20,"FB",22,"LED+"]
[null,21,"PWM",21,"NC"]
[null,22,"CP2",20,"NC"]
[null,23,"CP1",19,"LED-"]
[null,24,"AVDD",18,"FB"]
[null,25,"PVDD",17,"PWM"]
[null,26,"AGND",16,"CP2"]
[null,27,"VCOMH",15,"CP1"]
[null,28,"VCOML",14,"AVDD"]
[null,29,"PCDH",13,"PVDD"]
[null,30,"PCDL",12,"AGND"]
[null,31,"DUMMY",11,"VCOMH"]
[null,32,"DUMMY",10,"VCOML"]
[null,33,"DUMMY",9,"PCDH"]
[null,34,"DUMMY",8,"PCDL"]
[null,35,"CP8",7,"NC"]
[null,36,"CP7",6,"CP8"]
[null,37,"CP6",5,"CP7"]
[null,38,"CP5",4,"CP6"]
[null,39,"CP4",3,"CP5"]
[null,40,"CP3",2,"CP4"]
[null,null,null,1,"CP3"]

{"sheet":"FORMATS","index":30,"n_rows":28,"n_cols":4,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["CIF: Common Intermediate Format"]
[]
[]
[null,"FORMAT","NTSC","PAL"]
[null,"SQCIF","-","128 x 96"]
[null,"QCIF","176 x 120","176 x 144"]
[null,"QCIF+","176 x 220","176 x 220"]
[null,"CIF","352 x 240","352 x 288"]
[null,"VGA","640 x 480","-"]
[null,"WVGA","800 x 480"]
[null,"SVGA","800 x 600"]
[null,"WSVGA","1024 x 600"]
[null,"XGA","1024 x 768"]
[null,"WXVGA","1200 x 600"]
[null,"WXGA","1280 x 768"]
[null,"SXGA","1280 x 1024"]
[null,"UXGA","1600 x 1200"]
[null,"Full HD","1920 x 1080"]
[null,"qVGA","240 x 320","?"]
[null,"qqVGA","160 x 120"]
[null,"LqVGA","320 x 240"]
[null,"wVGA","480 x 864"]
[null,"wqVGA","240 x 432"]
[null,"hVGA","320 x 480"]
[null,"nHD","360 x 640"]
[]
[null,"4CIF","704 x 480","704 x 576"]
[null,"D1","720 x 480","720 x 576"]

{"sheet":"List1","index":31,"n_rows":49,"n_cols":2,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["LINK"]
[null,"Dots"]
["UG-2864AMBAG01.pdf"]
["JHD24064C"]
["JHD529"]
["V320P243282WSI7TB"]
["JHD12864J"]
["20T202DA1E"]
["EGO571M1"]
["JHD657"]
["JHD636"]
["JHD162P"]
["JHD639"]
["JHD12864H"]
["JHD756"]
["JHD12232D"]
["LQ035NC111"]
["JHD240128D / SHZJ2058"]
["LM6060C"]
["JHD12864C"]
["JHD613"]
["JHD204A.pdf"]
["TG12864R-04 VER:00"]
["JHD12864E"]
["LM2068E"]
["ADT-12232V10","122x32"]
["HSD070I651.pdf"]
["OCM128128-2.pdf"]
["TFT1N4609-E"]
["ERC12864F7-4"]
["JCTTQ2437PS01-T01.pdf"]
["KXM12864F-3.pdf"]
["WXCAT24-TSI.pdf"]
["HSD070IDW1-A.pdf"]
["TFT1N4633-E.pdf"]
["JHD508.pdf","128x64"]
["CT05568R.pdf"]
["TTW4070076.pdf"]
["LM6029ACW"]
["FH23-611S-0.3SHW.pdf"]
["JHD735 Model (1)"]
["TTW4070093.pdf"]
["JM320240A Model (1)"]
["TM240320A0NFWG%20SPEC%20V1.0.pdf"]
["JHD910 JHD901 V1.0 Model (1)"]
["EGO320240-1.pdf"]
["LPST128064A00-AB.pdf"]
["TM240320QNFWUG4-2"]
["TMT035DNAFWU24-2"]